## The Project Gutenberg eBook of Twine crochet work, with illustrations

This eBook is for the use of anyone anywhere in the United States and most other parts of the world at no cost and with almost no restrictions whatsoever. You may copy it, give it away or re-use it under the terms of the Project Gutenberg License included with this eBook or online at www.gutenberg.org. If you are not located in the United States, you will have to check the laws of the country where you are located before using this eBook.

Title: Twine crochet work, with illustrations

Compiler: active 1883-1884 Marie Louise Kerzman

Release date: December 5, 2025 [eBook #77404]

Language: English

Original publication: New York: Henry Bristow, 1883

Other information and formats: www.gutenberg.org/ebooks/77404

Credits: Charlene Taylor, Chris Miceli, and the Online Distributed Proofreading Team at https://www.pgdp.net (This file was produced from images generously made available by The Internet Archive/American Libraries.)

*** START OF THE PROJECT GUTENBERG EBOOK TWINE CROCHET WORK, WITH ILLUSTRATIONS ***
TRANSCRIBER’S NOTE

Some minor changes to the text are noted at the end of the book.

[Pg 1]

# TWINE
CROCHET WORK,
WITH ILLUSTRATIONS.
Second Edition. Enlarged.

COMPILED AND EDITED

BY

MARIE LOUISE KERZMAN.

PUBLISHED BY

HENRY BRISTOW,

296 Fulton St., Brooklyn, N. Y.

[2]

Entered according to Act of Congress, in the year 1883,
By HENRY BRISTOW,
the Office of the Librarian of Congress, Washington, D. C.

[3]

## INTRODUCTION TO SECOND EDITION.

The first edition of No. 2 of our Crochet Series was necessarily hurried, and issued out of its regular order, in compliance with a very general demand for lambrequin designs. While its success has been gratifying, there were some defects in the work, which has decided us to re-issue it under its present form. It has been carefully re-written, so as to follow the very full instructions found in No. 1. The number of designs have been doubled by the addition of some very attractive patterns for lambrequins.

Three numbers of the Series have been issued, as follows:

No. 1.—HOW TO CROCHET.

With full explanations of all Crochet Stitches, and numerous illustrations.

No. 2.—LAMBREQUIN DESIGNS.

Especially adapted for Twine. Illustrated. (Second Edition; Enlarged.)

No. 3.—MISCELLANEOUS DESIGNS.

Tidies, Mats and Spreads. Illustrated.

[4]

## TWINE CROCHET WORK.

The use of twine in fancy work has introduced a material that can be employed extensively in household decoration, and has brought the crochet needle into greater requisition than ever before. Many of those articles that contribute so much to the attractiveness of a home can be made of twine at comparatively little cost. It can be made in colors and of different sizes, and on account of its durability, cheapness and beauty, is considered by many superior to macramé work. By a judicious selection of shades, and a tasteful combination of trimmings, a large assortment of which are sold for that purpose, consisting of silk and plush balls of various shapes and colors, ribbon, etc., a great variety of articles may be fashioned which are at once both beautiful and effective, such as, for instance, window, mantel, fable and bracket lambrequins, scarfs for chairs and tables, covers for sofa pillows and ottomans, toilet and dinner mats, hand-bags, etc., etc., etc.

[5]

## DESCRIPTION OF TERMS USED IN CROCHET.

Chain Stitch.—Make a loop of twine, and draw the twine through each loop thus made, until the chain is of the required length.

Close Chain Stitch.—Insert the hook in loop of preceding row, and draw twine through both this loop and the loop on the needle at the same time.

Single Crochet.—Pass the hook through a loop of the last row, bring twine through, throw the twine around the needle and draw it through the two loops on the needle.

Double Crochet.—Turn the twine around the needle once, pass the hook through a loop of preceding row, bring twine through, throw the twine around the needle and draw it through two loops, turn the twine again around the needle and draw it through the two next loops.

Treble.—Turn the twine twice around the needle, work as double crochet, bringing twine through two loops three times.

Double Double Crochet.—Turn twine three times around the needle, work as double crochet, bringing twine through two loops four times.

Slip Stitch.—This stitch is used in joining. Take the hook from the last loop worked, pass it through the loop where the work has to be joined; then take the first loop spoken of and draw it through.

* The above are the primitive or foundation stitches, of which all fancy stitches are modifications or combinations.

[6]

### TWINE.

The best twine for crocheting is what is known as seine or macramé cotton twine, and is sold by numbers; 6 and 9, the finer numbers, are used for tidies, etc.; 12, 16 and 20 for lambrequins. Care should be taken in purchasing the twine, to get the best quality, as there are several grades made; that having a cream color, bordering on écru, makes the best work.

### NEEDLES.

A five-inch bone needle, even and smooth, is considered the best for crocheting with twine.

### ABBREVIATIONS USED IN DIRECTIONS.

st. | Stitch.
ch. st. | Chain Stitch.
cl. ch. st. | Close Chain Stitch.
s. c. | Single Crochet.
d. c. | Double Crochet.
t. | Treble.
d. d. c. | Double Double Crochet.
sl. st. | Slip Stitch.

* — * means to repeat the directions between the stars as often as told, as, for example: * 1 s.c., 1 ch.st. * 5 times, means to crochet 1 single crochet and 1 chain stitch until you have 5 alternate single crochet stitches and 5 chain stitches.

[7]

## LAMBREQUIN DESIGN No. 1.

### DIRECTIONS.

Make a chain of 43 stitches.

1st row.—3 d.c. in 4th ch.st., 3 ch.st., miss 1 ch.st., 3 d.c. in next ch.st., 9 ch.st., miss 11, 3 d.c. in 12th, 3 ch.st., miss 1, 3 d.c. in next ch.st., miss 3, 1 d.c. in 4th, miss next 3, 3 d.c. in 4th, 3 ch.st., miss 1, 3 d.c. in next ch.st., 9 ch.st., miss 11, 3 d.c. in 12th, 3 ch.st., miss 1, 3 d.c. in next ch.st. Turn.

2d row.—3 ch.st., 3 d.c. around chain of 3 between the two 3 d.c. of last row, 3 ch.st., 3 d.c. around same chain, 9 ch.st., 3 d.c., 3 ch.st., 3 d.c. around next ch. of 3, 1 d.c. in d.c. of last row, 3 d.c., 3 ch.st., 3 d.c. around next ch. of 3, 9 ch.st., 3 d.c., 3 ch.st., 3 d.c. around following ch. of 3. Turn.

[8]

3d. row.—3 ch.st., 2 d.c. in last d. crochet of 2d row, 3 ch.st., 3 d.c. around next ch. of 3, 3 ch.st., 3 d.c. around same ch., 4 ch.st., fasten in 5th ch.st. of chains of 2d and 1st rows, 4 ch.st., 3 d.c. around next ch. of 3, 3 ch.st., 3 d.c. around same ch., 1 d.c. in d.c. of last row, 3 d.c., 3 ch.st., 3 d.c. around following ch. of 3, 4 ch.st., fasten in 5th ch.st. of chains of 2d and 1st rows, 4 ch.st., 3 d.c. around next ch. of 3, 3 ch.st., 3 d.c. around same chain. Turn.

4th row.—3 ch.st., 3 d.c. around ch. of 3 of 3d row, 3 ch.st., 3 d.c. around same ch., 9 ch.st., 3 d.c. around next ch. of 3, 3 ch.st., 3 d.c. around same chain, 1 d.c. in d.c. of last row, 3 d.c., 3 ch.st., 3 d.c. around ch. of 3, 9 ch.st., 3 d.c. around next ch. of 3, 3 ch.st., 3 d.c. around same ch., then 3 ch.st., 3 d.c. around next ch. of 3. Turn.

5th row.—3 ch.st., 2 d.c. in last d.c. of preceding row (4th row), 3 ch.st., 3 d.c. around next ch. of 3, 3 ch.st., 3 d.c. around next ch. of 3, 3 ch.st., 3 d.c. around same ch., 9 ch.st., 3 d.c., 3 ch.st., 3 d.c., 1 d.c., 3 d.c., 3 ch.st., 3 d.c., 9 ch.st., 3 d.c., 3 ch.st., 3 d.c. Turn.

6th row.—3 ch.st., 3 d.c. around next ch. of 3, 3 ch.st., 3 d.c. around same, 9 ch.st., 3 d.c., 3 ch.st., 3 d.c., 1 d.c., 3 d.c., 3 ch.st., 3 d.c., 9 ch.st., 3 d.c., 3 ch.st., 3 d.c. then 3 ch.st., 3 d.c. around next ch. of 3, 3 ch.st., 3 d.c. around next ch. of 3. Turn.

7th row.—3 ch.st., 2 d.c. in last d.c. of last row, 3 ch.st., 3 d.c. around ch. of 3, 3 ch.st., 3 d.c. around next ch. of 3, 3 ch.st., † 3 d.c. around next ch. of 3, 3 ch.st., 3 d.c. around same, 4 ch.st., fasten in 5th ch.st. of chains of two last rows. 4 ch.st.,[9] 3 d.c. around next ch. of 3, 3 ch.st., 3 d.c. around same ch., 1 d.c. in d.c., 3 d.c., 3 ch.st., 3 d.c. around next ch. of 3, 4 ch.st., fasten in 5th ch.st. of chains of 2 last rows, 4 ch.st., 3 d.c., 3 ch.st., 3 d.c. around next ch. of 3. Turn.

8th row.—3 ch.st., 3 d.c. around ch. of 3, 3 ch.st., 3 d.c. around same, 9 ch.st., etc., as before. Then at the point work 3 ch.st., 3 d.c. around next ch. of 3, 3 ch.st., 3 d.c. around next ch. of 3, 3 ch.st., 3 d.c. around last ch. Turn.

9th row.—3 ch.st., 2 d.c. in last double crochet of last row, 3 ch.st., 3 d.c. around next ch. of 3, 3 ch.st., 3 d.c. around next ch. of 3, 3 ch.st., 3 d.c. around next ch. of 3, 3 ch.st. Crochet to the end of the row, as before.

10th row.—3 ch.st., 3 d.c., 3 ch.st., 3 d.c., 9 ch.st., etc. Then, at beginning of point, work 3 ch.st., 3 d.c. around next ch. of 3, 3 ch.st., 3 d.c. around next ch., 3 ch.st., 3 d.c. around following ch., 3 ch.st., 3 d.c. around next ch. Turn.

11th row.—3 ch.st., 2 d.c. in last d.c. of preceding row, 3 ch.st., 3 d.c., 3 ch.st., 3 d.c., 3 ch.st., 3 d.c., 3 ch.st., 3 d.c., 3 ch.st., then continue working like 7th row from † to end of the row.

12th row.—3 ch.st., 3 d.c. around ch. of 3, 3 ch.st., 3 d.c. around same ch., 9 ch.st., etc., as before, to beginning of point. Then * 3 ch.st., 3 d.c. around next ch. of 3 *. Repeat 4 times.

13th row.—3 ch.st., 3 d.c. in last d.c. of last row, * 1 s.c., 1 h.d.c., 3 d.c. around next ch. of 3*. Repeat 4 times, then work as usual to the end, making it the required length.

Fasten the fringe in every other stitch around the points of the Lambrequin.

[10]

## LAMBREQUIN DESIGN No. 2.

### DIRECTIONS.

Make a chain of 49 stitches.

1st row.—4 d.c. in 3d ch.st., 1 ch.st., 3 d.c. in same, miss next 4 ch.st., 2 d.c. in 5th, miss 2 ch.st., 4 d.c. in 3d, make 1 ch.st., 3 d.c. in same 3d ch.st., 7 ch.st., miss 10, 4 d.c. in 11th, 1 ch.st., 3 d.c. in same, miss 4 ch.st., 2 d.c. in 5th, miss next 2, 4 d.c. in 3d, 1 ch.st., 3 d.c. in same, 7 ch.st., miss 10, 4 d.c. in 11th, 1 ch.st., 3 d.c. in same, miss next 4 ch.st., 2 d.c. in 5th, miss next 2, 4 d.c. in 3d, 1 ch.st. 3 d.c. in same. Turn.

2d row.—3 ch.st., * 4 d.c. around next ch. of 1, 1 ch.st., 3 d.c. around same ch., 2 d.c. between next 2 d.c. of last row, 4 d.c. around next ch. of 1, 1 ch.st., 3 d.c. around same ch., 7 ch.st.; * repeat once; then 4 d.c. around next ch. of 1, 1 ch.st., 3 d.c. around same ch., 2 d.c. between next 2 d.c., 4[11] d.c. around next ch. of 1, 1 ch.st., 3 d.c. around same ch. Turn.

3d row.—3 ch.st., * 4 d.c. around next ch. of 1, 1 ch.st., 3 d.c. around same ch. 2 d.c. between next 2 d.c., 4 d.c. around next ch. of 1, 1 ch.st., 3 d.c. around same ch., 4 ch.st., fasten to chains of 2d and 1st rows by passing the hook through 4th ch.st. of ch. of 1st row, making at the same time a s.c.; 3 ch.st.; * repeat once; then 4 d.c. around next chain of 1, 1 ch.st., 3 d.c. around same ch., 2 d.c. between 2 d.c., 4 d.c. around next ch. of 1, 1 ch.st., 3 d.c. around same ch. Turn.

4th row.—3 ch.st., 4 d.c., 1 ch.st., 3 d.c., 2 d.c., 4 d.c., 1 ch.st., 3 d.c., 7 ch.st., 4 d.c. around next ch. of 1, 1 ch.st., 3 d.c. around same ch., 2 d.c., 4 d.c., 1 ch.st., 3 d.c., 7 ch.st., 4 d.c., 1 ch.st., 3 d.c., 2 d.c., 4 d.c., 1 ch.st., 3 d.c.; then 10 d.c. around the ch. of 3, which is at the bottom edge of the work; fasten in 1st d.c. of 1st row. Turn.

5th row.—1 cl.ch.st., 3 ch.st. in every other d.c. of the 10 d.c. last made, * 4 d.c. around next ch. of 1, 1 ch.st., 3 d.c. around same ch., 2 d.c. between next 2 d.c., 4 d.c. around next ch. of 1, 1 ch.st., 3 d.c. around same ch., 7 ch.st.; * repeat, but at the last repetition stop at 7 ch.st.

The work is continued by always repeating the rows described, from 2d row.

Fasten the fringe in every other stitch at the bottom edge of the work.

[12]

## LAMBREQUIN DESIGN No. 3.

### DIRECTIONS.

Make a chain of 43 stitches.

1st row.—3 d.c. in the 5th ch.st.; 3 ch.st.; 3 d.c. in same 5th ch.st.; 9 ch.st.; miss 12; 3 d.c. in 13th; 3 ch.st., 3 d.c. in same, 9 ch.st., miss 12, 3 d.c. in 13th, 3 ch.st., 3 d.c. in next stitch, 7 ch.st., miss 4, fasten in 5th with a s.c. Turn.

2d row.—3 ch.st., 12 d.c. around last chain of 7, * 3 d.c., 3 ch.st., 3 d.c. around next ch. of 3, 4 ch.st., fasten in 5th ch.st. of ch. of last row, 4 ch.st.; * repeat once, then make 3 d.c., 3 ch.st., 3 d.c. around last chain of 3. Turn.

3d row.—2 ch.st., 3 d.c., 3 ch.st., 3 d.c. around next chain of 3, 9 ch.st., 3 d.c., 3 ch.st., 3 d.c. around next ch. of 3, 9 ch.st., 3 d.c., 3 ch.st., 3 d.c. around next ch. of 3, * 1 d.c. in next d.c., 1 ch.st. * Repeat 10 times; at the end fasten in 1st st. of foundation chain. Turn.

[13]

4th row.—3 ch.st., * 1 d.c. around ch. of 1 of last row, 2 ch.st. * Repeat 9 times. Then 3 d.c., 3 ch.st., 3 d.c. around next ch. of 3, etc. Work to the end as in 2d row. Turn.

5th row.—2 ch.st., 3 d.c., 3 ch.st., 3 d.c., 9 ch.st., 3 d.c., 3 ch.st., 3 d.c., 9 ch.st. 3 d.c., 3 ch.st., 3 d.c.; then 1 ch.st., * 1 d.c. around next ch. of 2, 3 ch.st. *; repeat 9 times. Turn.

6th row.—* 5 ch.st., 1 s.c. around next ch. of 3 *; repeat 8 times; then 5 ch.st., 1 s.c. around next ch. of 1, 3 d.c., 3 ch.st., 3 d.c. around next ch. of 3, 4 ch.st., etc., like 4th row. Turn.

7th row.—2 ch.st., 3 d.c., 3 ch.st., 3 d.c., 9 ch.st., 3 d.c., 3 ch.st., 3 d.c., 9 ch.st., 3 d.c., 3 ch.st., 3 d.c.; then 7 ch.st., fasten around 2d chain of 5 of 6th row. Turn.

8th row.—3 ch.st., 12 d.c. around last ch. of 7; go on working like 2d row. Turn.

9th row.—Work up to scallop like 3d row; then make * 1 d.c. in next d.c., 1 ch.st.; * repeat 11 times, then fasten around 3d ch. of 5 of 6th row. Turn.

10th row.—3 ch.st., * 1 d.c. around next ch. of 1 of last row, 2 ch.st. *; repeat ten times; work to the end of row, like 4th row.

11th row.—Work up to the scallop like 5th row, then 1 ch.st., * 1 d.c. around next ch. of 2, 3 ch.st., * repeat 11 times, fasten in 4th ch. of 5 of 6th row. Turn.

12th row.—* 5 ch.st., 1 s.c. around next ch. of 3 *; repeat 10 times; then continue to work 5 ch.st.,[14] 1 s.c. around next ch. of 1, 3 d.c., etc., like 6th row.

The following scallops are worked after directions of 2d scallop, as the foundation chain make a difference in the number of stitches of the 1st.

Fasten fringe in the chains of 5 on the edge of every scallop.

## LAMBREQUIN DESIGN No. 4.

### DIRECTIONS.

Make a chain of 44.

1st row.—Miss 4 ch.st., make 1 d.c. in each of the next 7 ch.st., 8 ch.st., miss 8, 1 d.c. in the following 8 ch.st., 8 ch.st., miss 8, 1 d.c. in the following 8 ch.st. Turn.

[15]

2d row.—3 ch.st., miss 1 d.c., make 1 d.c. in the next 7 d.c. of last row, 8 ch.st., 1 d.c. in the next 8 d.c., 8 ch.st.; 1 d.c. in the next 8 d.c., 7 ch.st., fasten in last stitch of foundation. Turn.

3d. row.—13 s.c. around ch. of 7 of last row; 1 ch.st., * 1 d.c. in next 8 d.c., 4 ch.st., fasten in middle st. of both preceding chains, 4 ch.st.; * repeat once, then 1 d.c. in next 8 d.c. Turn.

4th row.—3 ch.st., 1 d.c. in next 7 d.c., 8 ch.st., 1 d.c. in next 8 d.c., 8 ch.st., 1 d.c. in next 8 d.c., 7 ch.st., fasten on end of 3d in the 1 ch.st. Turn.

5th row.—13 s.c. around ch. of 7 of last row, 1 ch.st., 8 d.c., 8 ch.st., 8 d.c., 8 ch.st., 8 d.c. Turn.

6th row.—3 ch.st., 7 d.c., 8 ch.st., 8 d.c., 8 ch.st., 8 d.c., 7 ch.st., fasten on end of 5th row in the 1 ch.st. Turn.

7th row.—13 s.c. around ch. of 7, 1 ch.st., 8 s.c., 4 ch.st., fasten in middle st. of 2 preceding chains, 4 ch.st., 8 d.c., 4 ch.st., fasten as before, 4 ch.st., 8 d.c. Turn.

8th row.—3 ch.st., 7 d.c., 8 ch.st., 8 d.c., 8 ch.st., 8 d.c., 7 ch.st., fasten in the 1 ch.st. Turn.

9th row.—13 s.c. around chain of 7, 1 ch.st., 8 d.c., 8 ch.st., 8 d.c., 8 ch.st., 8 d.c. Turn.

10th row.—3 ch.st., 7 d.c., 8 ch.st., 8 d.c., 8 ch.st., 8 d.c.; then 7 ch.st.; fasten in chain of 1. Turn. 7 s.c. around half of ch. of 7, turn, * 7 ch.st., fasten in 7th s.c. of next scallop *; repeat 3 times, turn * 13 s.c. around ch. of 7 *; repeat twice, then 7 s.c. around half of next ch. of 7, turn, * 7 ch.st., fasten in 7th s.c. of next scallop *; repeat twice, turn, * 14 s.c. around next ch. of 7; * repeat once, 7 s.c. around half of next ch. of 7, turn, * 8 ch.st.,[16] fasten in 7th s.c. of next scallop *; repeat once, turn, 15 s.c. around ch. of 8 last worked, 8 s.c. around half of next ch. of 8, turn, 9 ch.st., fasten in 8th s.c. of next scallop, turn, 16 s.c. around ch. last worked, 7 s.c. around remaining half of next ch. of 8, 7 s.c. around remaining half of next ch. of 7, 6 s.c. around the remaining half of the next ch. of 7, 6 s.c. around the remaining half of the next ch. of 7.

11th row.—1 ch.st., 8 d.c., 4 ch.st., fasten as before, 4 ch.st., 8 d.c., 4 ch.st., fasten, 4 ch.st., 8 d.c.

Repeat entire work from second row.

After having reached the entire length of the lambrequin, work 8 d.c. in the end of every other row on the upper edge of the lambrequin, fastening by 1 s.c. in the intervening rows.

## FRINGE.

All the Lambrequin designs given are finished with a fringe, which is easily made, and the following directions will apply to all: Cut the twine twice the required length, double in center; take two pieces together, put the needle through the stitch nearest the edge, and with the hook catch the twines in center and draw through until a loop is formed on the opposite side; pass the needle through the loop and draw the four ends through, then pull tight.

[17]

## LAMBREQUIN DESIGN No. 5.

### DIRECTIONS.

Make a chain of the required length.

1st row.—4 ch.st., 3 t. in last st. of foundation chain, 2 ch.st., 3 t. in same ch.st., * 6 ch.st., miss 8, 3 t., 3 ch.st., 3 t. in 9th *; repeat to the end of row; turn with 2 cl.ch.st. in last 2 t.

2d row.—2 ch.st., 4 t., 2 ch.st., 4 t. around next ch. of 2, separating the two 3 t. of last row, * 7 ch.st., 4 t., 2 ch.st., 4 t. around next 2 ch.st. *; repeat to end of row; turn with 3 cl.ch.st. in last 3 t.

3d row.—5 t., 3 ch.st., 5 t. around next chain of 2, * 7 ch.st., 5 t., 3 ch.st., 5 t. around next ch. of 3 *; repeat to end of row. Turn, with 4 cl.ch.st. in last 4 t.

4th row.—2 ch.st., 6 t., 3 ch.st., 6 t. around next chain of 3, * 4 ch.st., fasten in the middle of the chains of two preceding rows, 3 ch.st., 6 t., 3 ch.st., 6 t. around next ch. of 3 *; repeat to end of row. Turn, with 3 cl.ch.st.

[18]

5th row.—1 ch.st., 11 t. around next ch. of 3, * 4 ch.st., 11 t. around next ch. of 3 *; repeat to end of row. Turn.

6th row.—3 ch.st., miss 1 t., 1 d.c., followed by 1 ch.st. in each of next 9 t., * 1 s.c. in last t. of scallop, 4 cl.ch.st. in next 4 ch.st., 1 s.c. in next t., 1 d.c., followed by 1 ch.st. in each of next 9 t. *; repeat to end of row.

Heading.—1 s.c. in each st. of foundation chain. Turn.

2d row.—3 ch.st., fasten in every other s.c. of last row. Turn.

3d row.—*3 ch.st., fasten in middle stitch of chain of 3 of last row *; repeat to end of row. Turn, with 1 ch.st.

4th row.—1 s.c. in every stitch of last row.

5th row.—1 ch.st., 1 d.c., 1 ch.st., 1 d.c., 1 ch.st., 1 d.c., all worked in next 2d st. of last row, 1 ch.st., miss next s.c., 1 s.c. in next s.c. *; repeat to end of row.

[19]

## LAMBREQUIN DESIGN No. 6.

### DIRECTIONS.

Make any number of chain stitches divisible by 9, half as long again as desired when finished, as it takes up in working.

1st row.—* 1 d.c. in each of first 9 ch.st.; 9 ch.st.; miss 8; 1 d.c. in next 9 ch.st. * Repeat to end of row, finishing with 9 d.c.

Every row has to be worked on the right side of the work; consequently the twine has to be broken at the end of every row.

2d row.—* 9 d.c.; 9 ch.st. * Repeat to the end of the row, finishing with 9 d.c.

3d row.—* 9 d.c.; 4 ch.st.; 1 s.c. through 5th ch.st. of 2d and 3d rows, drawing tightly together; 4 ch.st. * Repeat.

4th row.—* 9 d.c.; 9 ch.st. * Repeat.

5th row.—* 9 d.c.; 9 ch.st. * Repeat.

6th row.—* 9 d.c.; 9 ch.st. * Repeat.

7th row.—* 9 d.c.; 4 ch.st.; 1 s.c. through 5th ch.st. of chain of 5th and 6th rows; 4 ch.st. * Repeat.

[20]

8th row.—Repeat 5th row.

9th row.—d.c. to end of row.

Heading.—* 6 d.c. in 3d d.c.; miss 2; fasten on 3d by 1 s.c. * Repeat.

To finish it off on the bottom, work * 10 t. in 5th d.c.; 1 s.c. in 9th d.c.; 4 ch.st.; 1 s.c. in 5th ch.st. of chain of the last row; 4 ch.st.; 1 s.c. in first of the next 9 d.c. * Repeat.

The fringe is put in every other loop of the edge of this last described row.

## LAMBREQUIN DESIGN No. 7

### DIRECTIONS.

Make a chain of 28 stitches.

1st row.—3 d.c. in 4th ch.st.; 3 ch.st.; 3 d.c. in next ch.st.; 7 ch.st.; miss 9 ch.st.; make 3 d.c. in the 10th; 3 ch.st.; 3 d.c. in next ch.st.; 7 ch.st.; miss 9 ch.st.; work 3 d.c. in the 10th; 3 ch.st.; 3 d.c. in the next ch.st., which should be the last st. of foundation chain.

[21]

2d row.—Turn; 3 ch.st.; 3 d.c. around chain made by 3 ch.st. in last row; 3 ch.st.; 3 d.c. around same chain; 7 ch.st.; 3 d.c. around the next chain of 3; 3 ch.st.; 3 d.c. around the same chain; 7 ch.st.; 3 d.c. around the next chain of 3; 3 ch.st.; 3 d.c. round the same chain; 7 ch.st.; fasten to end of 1st row; 12 s.c. in chain made by 7 ch.st.

3d row.—1 ch.st.; 3 d.c. around last chain of 3 in 2d row; 3 ch.st.; 3 d.c. around the same chain; 3 ch.st.; 1 s.c. through the middle stitch of ch. of 7 of 1st and 2d rows; 3 ch.st.; 3 d.c. around next chain of 3; 3 ch.st.; 3 d.c. around same chain; 3 ch.st.; 1 s.c. through middle stitch of next ch. of 7 of 1st and 2d rows; 3 ch.st.; 3 d.c. around the next chain of 3; 3 ch.st.; 3 d.c. around the same chain.

4th row.—Turn the work; 3 ch.st.; 3 d.c. around 3 ch. of 3; 3 ch.st.; 3 d.c. around same chain; 7 ch.st.; 3 d.c. around next ch. of 3; 3 ch.st.; 3 d.c. around same chain; 7 ch.st.; 3 d.c. around next ch. of 3; 3 ch.st.; 3 d.c. around same chain; 7 ch.st.; fasten to loop made by the 1 ch.st. at beginning of 3d row; 12 s.c. around 2d scallop.

5th row.—1 ch.st.; 3 d.c. around chain of 3; 3 ch.st.; 3 d.c. around same; 7 ch.st.; 3 d.c. around next chain of 3; 3 ch.st.; 3 d.c. around the same; 7 ch.st.; 3 d.c. around next chain of 3; 3 ch.st.; 3 d.c. around same.

6th row.—Turn the work; 3 ch.st.; 3 d.c. around chain of 3; 3 ch.st.; 3 d.c. around same chain; 7 ch.st.; 3 d.c.; 3 ch.st.; 3 d.c.; 7 ch.st.; 3 d.c.; 3 ch.st.; 3 d.c.; 7 ch.st.; fasten to loop made by the 1 ch.st. at beginning of 5th row; turn; 6 s.c.; turn; 7 ch.st.;[22] fasten in middle of 2d scallop at bottom of work; 7 ch.st.; fasten in middle of next scal.; turn; 12 s.c. around chain of 7; 6 s.c. around next 7 ch.st.; turn; 7 ch.st.; fasten in scal.; turn; 12 s.c. around 7 ch.st.; 6 s.c. around half finished scal.; 6 s.c. around next half scal.; 1 ch.st.; 3 d.c. around chain of 3 of preceding row; 3 ch.st.; 3 d.c. around same chain; 3 ch.st.; 1 s.c. through middle stitch of ch. of 5th and 6th rows; 3 ch.st.; 3 d.c. around next chain of 3; 3 ch.st.; 3 d.c. around same chain; 3 ch.st.; 1 s.c. in middle stitch of ch. of 5th and 6th rows; 3 ch.st.; 3 d.c. around next chain of 3; 3 ch.st.; 3 d.c. around same chain.

Fasten fringe in every other stitch of the bottom edge.

## LAMBREQUIN DESIGN No. 8.

### DIRECTIONS.

Make a chain of 30 stitches.

1st row.—3 d.c. in 4th st. of chain; 3 ch.st.; 3 d.c. in same (4th) st.; 7 ch.st.; miss 10 ch.st.; put 3[23] d.c. in 11th; 3 ch.st.; 3 d.c. in same; miss 3 ch.st.; put 3 d.c. in 4th; 3 ch.st.; 3 d.c. in same; 7 ch.st.; 3 d.c. in last of foundation chain; 3 ch.st.; 3 d.c. in same.

2d row.—Turn; 3 ch.st.; 3 d.c. around chain of 3 of last row; 3 ch.st.; 3 d.c. around same chain; 7 ch.st.; 3 d.c. around next chain of 3; 3 ch.st.; 3 d.c. around same chain; 3 d.c. around next chain of 3; 3 ch.st.; 3 d.c. around same chain; 7 ch.st.; 3 d.c. around next chain of 3; 3 ch.st.; 3 d.c. around same chain; 3 ch.st.

3d row.—Turn; crochet to end of row as before, then 3 ch.st.; 3 d.c. around chain of 3 of last row.

4th row.—3 ch.st.; 3 d.c. in chain of 3 of 3d row; 3 ch.st.; then 3 d.c. in next chain of 3; 3 ch.st., etc. Crochet to end of, as before.

5th row.—3 ch.st.; 3 d.c. around chain of 3 of preceding row; 3 ch.st.; 3 d.c. around same; 7 ch.st.; 3 d.c. around next; 3 ch.st.; 3 d.c. around same; 3 d.c. around next; 3 ch.st.; 3 d.c. around same; 7 ch.st.; 3 d.c. around next; 3 ch.st.; 3 d.c. around same; 3 ch.st.; 3 d.c. around next ch. of 3, which is in the point; 3 ch.st.; 3 d.c. around next ch.

6th row.—3 ch.st.; 3 d.c.; 3 ch.st.; 3 d.c.; 3 ch.st.; finish to the end of row, as usual.

7th row.—Crochet as usual to beginning of point, then 3 ch.st.; 3 d.c.; 3 ch.st.; 3 d.c.; 3 ch.st.; 3 d.c.

8th row.—3 ch.st.; 3 d.c., etc.

9th row.—Crochet as usual to beginning of point, then 3 ch.st.; 3 d.c.; 3 ch.st.; 3 d.c.; 3 ch.st.; 3 d.c.; 3 ch.st.; 3 d.c.

10th row.—3 ch.st.; 3 d.c.; 3 ch.st.; 3 d.c.; 3 ch.st.; 3 d.c.; 3 ch.st.; 3 d.c.; then as usual to the end,[24] making it the required length. Crochet as a heading, 7 d.c. around 3 ch.st. at the top, fastening each one down before another.

The fringe must be fastened in every other stitch of the bottom edge.

## LAMBREQUIN DESIGN No. 9.

### DIRECTIONS.

Make a chain of 39 stitches.

1st row.—2 d.c. in 4th st. of ch.; 1 ch.st.; 2 d.c. in same (4th) st.; miss 2 ch.st.; put 2 d.c. in 3d ch.st.; 1 ch.st.; 2 d.c. in same 3d ch.st.; 7 ch.st.; miss 8 ch.st.; put 2 d.c. in 9th ch.st.; 1 ch.st.; 2 d.c. in same; miss 3 ch.st.; put 2 d.c. in 4th; 1 ch.st.; 2 d.c. in same 1 ch.st.; miss 2 ch.st.; put 1 d.c. in next 12 ch.st.; 3 ch.st.; 3 d.c. in last stitch of chain; 1 ch.st.; 1 t.c. in 1 last st. of chain; 4 ch.st. and turn.

[25]

2d row.—4 d.c. around last 1 ch.st. of 1st row; 2 ch.st.; 4 d.c. around next 3 ch.st.; 2 ch.st.; miss next 2 d.c.; make 1 d.c. in following 10 d.c. of 1st row; 1 ch.st.; miss 1 ch.st.; 2 d.c. around next chain of 1, which separates the 4 d.c. coming together in last row; 1 ch.st.; 2 d.c. around same chain of 1; 2 d.c. around next chain of 1; 1 ch.st.; 2 d.c. in same chain; 7 ch.st.; 2 d.c. around next chain of 1; 1 ch.st.; 2 d.c. around same chain; 2 d.c. around next chain of 1; 1 ch.st.; 2 d.c. in same chain; 3 ch.st.; turn.

3d row.—2 d.c. around 1st chain of 1 of 2d row; 1 ch.st.; 2 d.c. around same chain; 2 d.c.; 1 ch.st.; 2 d.c. around next chain of 1; 3 ch.st.; 1 s.c. through 4th st. of chain of 1st and 2d row, drawing tightly together; 3 ch.st.; 2 d.c. around next chain of 1; 1 ch.st.; 2 d.c. around same chain; 2 d.c. around next chain of 1; 1 ch.st.; 2 d.c. around same chain; 1 ch.st.; 1 d.c. in 8 d.c. of preceding row; 2 ch.st.; 4 d.c. around 2 ch.st. of preceding row; 2 ch.st.; 4 d.c.; 2 ch.st.; 4 d.c.; 1 ch.st.; 1 t.; 4 ch.st.

4th row.—4 d.c. around last t. and d.c. of 3d row; 2 ch.st.; 4 d.c.; 2 ch.st.; 4 d.c.; 2 ch.st.; 4 d.c.; 2 ch.st.; miss 2; 1 d.c. in next 6 d.c. of 3d row; 1 ch.st.; 2 d.c. around next chain of 1; 1 ch.st.; 2 d.c. around same chain; 2 d.c. around next chain of 1; 1 ch.st.; 2 d.c. around same chain; 7 ch.st.; 2 d.c. around next chain of 1; 1 ch.st.; 2 d.c. around same chain; 2 d.c. around next chain of 1; 1 ch.st.; 2 d.c. in same chain; 3 ch.st.

5th row.—2 d.c.; 1 ch.st.; 2 d.c., as before; 2 d.c.; 1 ch.st.; 2 d.c. in next chain of 1; 7 ch.st.; 2 d.c.;[26] 1 ch.st.; 2 d.c.; 2 d.c.; 1 ch.st.; 2 d.c.; 1 ch.st.; 1 d.c. in 4 d.c. of preceding row; 2 ch.st.; 4 d.c.; 2 ch.st.; 4 d.c.; 2 ch.st.; 4 d.c.; 2 ch.st.; 4 d.c.; 2 ch.st.; 4 d.c.; 1 ch.st.; 1 t.; 4 ch.st.

6th row.—4 d.c. around last t. and d.c. of 5th row; 2 ch.st.; 4 d.c.; 2 ch.st.; 4 d.c.; 2 ch.st.; 4 d.c.; 2 ch.st.; 4 d.c.; 2 ch.st.; 4 d.c.; 2 ch.st.; miss next 2 d.c.; 1 d.c. in next 2 d.c. of 5th row; 1 ch.st.; 2 d.c. around next chain of 1; 1 ch.st.; 2 d.c. in same chain; 2 d.c. in next chain of 1; 1 ch.st.; 2 d.c. in same chain; 7 ch.st.; 2 d.c. around next chain of 1; 1 ch.st.; 2 d.c. around same chain; 2 d.c. around last chain; 1 ch.st.; 2 d.c. around same chain; 3 ch.st.

7th row.—2 d.c. around chain of 1; 1 ch.st.; 2 d.c. around same chain; 2 d.c. around next chain of 1; 1 ch.st.; 2 d.c. around same chain; 3 ch.st.; 1 s.c. through 4th st. of last 2 chains, drawing tightly together; 3 ch.st.; 2 d.c. around next chain of 1; 1 ch.st.; 2 d.c. around same chain; 2 d.c. around next chain of 1; 1 ch.st.; 2 d.c. around same chain; 1 ch.st.; miss 1 ch.st.; 1 d.c. in next 4 st. of last row; 2 ch.st.; 4 d.c.; 2 ch.st.; 4 d.c.; 2 ch.st.; 4 d.c.; 2 ch.st.; 4 d.c.; 2 ch.st.; 4 d.c.; 1 s.c. in d.c. of 6th row; turn.

8th row.—1 s.c. in each of 4 d.c. of preceding row; 4 d.c. around 3 ch.st. of 7th row; 2 ch.st.; 4 d.c.; 2 ch.st.; 4 d.c.; 2 ch.st.; 4 d.c.; 2 ch.st.; miss next 4 d.c.; 1 d.c. in next 6 st.; 1 ch.st.; 2 d.c. around chain of 1; 1 ch.st.; 2 d.c. around same chain; 2 d.c. around next chain of 1; 1 ch.st.; 2 d.c. around same; 7 ch.st.; 2 d.c. around next chain of 1; 1 ch.st.; 2 d.c. around same chain; 2 d.c. around next chain of 1; 1 ch.st.; 2 d.c. around same chain; 3 ch.st.

[27]

9th row.—2 d.c.; 1 ch.st.; 2 d.c. around chain of 1; 2 d.c.; 1 ch.st.; 2 d.c. around next chain of 1; 7 ch.st.; 2 d.c.; 1 ch.st.; 2 d.c. around chain of 1; 2 d.c. around next chain of 1; 1 ch.st.; 2 d.c. around same chain; 1 ch.st.; 1 d.c. in next 8 d.c.; 2 ch.st.; 4 d.c.; 2 ch.st.; 4 d.c.; 2 ch.st.; 4 d.c.; 1 s.c. in d.c. of 6th row; turn.

10th row.—1 s.c. in each of 4 d.c. of preceding row; 4 d.c. around next chain of 3 of 9th row; 2 ch.st.; 4 d.c.; 2 ch.st.; miss next 4 d.c.; make 10 d.c.; 1 ch.st.; 2 d.c.; 1 ch.st.; 2 d.c. around chain of 1; 2 d.c.; 1 ch.st.; 2 d.c. around next chain of 1; 7 ch.st.; 2 d.c.; 1 ch.st.; 2 d.c. around chain of 1; 2 d.c.; 1 ch.st.; 2 d.c. around last chain of 1; 3 ch.st.

These 10 rows are continually repeated, until the length of the lambrequin is reached.

## LAMBREQUIN DESIGN No. 10.

### DIRECTIONS.

Make a chain of 41 stitches.

1st row.—3 d.c. in 4th ch.st.; 3 ch.st.; 3 d.c. in[28] next st.; 9 ch.st.; miss 11; put 3 d.c. in 12th ch.st.; 3 ch.st.; 3 d.c. in next; miss 3 ch.st.; put 1 d.c. in each of next 3 ch.st.; miss 3 ch.st.; put 3 d.c. in 4th; 3 ch.st.; 3 d.c. in next; 9 ch.st.; miss 11; 3 d.c. in 12th ch.st.; 3 ch.st.; 3 d.c. in same st. of chain; 3 ch.st.

2d row.—3 d.c. around 1st chain of 3 between the two 3 d.c. of 1st row; 3 ch.st.; 3 d.c. around same; 4 ch.st.; 1 cl.ch.st. through 5th st. of chain in 1st row; 4 ch.st.; 3 d.c. around next chain of 3; 3 ch.st.; 3 d.c. around same; 1 d.c. in each of the d.c. of 1st row; 3 d.c. around next chain of 3; 3 ch.st.; 3 d.c. around same; 4 ch.st.; 1 cl.ch.st. through 5th st. of ch. of 1st row; 4 ch.st.; 3 d.c. around next chain of 3; 3 ch.st.; 3 d.c. around same; 5 ch.st.; fasten to beginning of preceding row. Turn 10 s.c. around last chain of 5.

Repeat these two rows until the desired length, then finish off the bottom with 12 trebles around chain of 3 at end of rows, always fastening before beginning the next one.

[29]

## LAMBREQUIN DESIGN No. 11.

### DIRECTIONS.

Make a chain of 35 stitches.

1st row.—3 d.c. in 4th ch.st., 3 ch.st., 3 d.c. in same st., fasten to next 3d st. of ch., 6 ch.st., miss 6 ch.st., 3 d.c. in 7th, 3 ch.st., 3 d.c. in same, fasten to next 3d ch.st., 6 ch.st., miss 6, put 3 d.c. in 7th, 3 ch.st., 3 d.c. in same, fasten to next 3d st., 6 ch.st., miss 6, 3 d.c. in 7th st. of ch., 3 ch.st., 3 d.c. in next ch.st., 5 ch.st., and turn.

2d row.—3 d.c. around next chain of 3, worked between the last 3 d.c. in preceding row, 3 ch.st., 3 d.c. around same, fasten around 1st st. of next chain of 6, 6 ch.st., 3 d.c. around next chain of 3, 3 ch.st., 3 d.c. around same ch., fasten, 6 ch.st., 3 d.c. around next chain of 3, 3 ch.st., 3 d.c. around[30] same chain, fasten, 6 ch.st., 3 d.c. around next chain of 3. 3 ch.st., 3 d.c. around same, work 6 ch.st., turn.

3d row.—3 d.c. around next chain of 3 of 2d row, 3 ch.st., 3 d.c. around same chain, fasten, 6 ch.st., 3 d.c., around next ch. of 3, 3 ch.st., 3 d.c. around same ch., fasten, 6 ch.st., 3 d.c. around next ch. of 3, 3 ch.st., 3 d.c. around same, fasten, 6 ch.st., 3 d.c. around next ch. of 3, 3 ch.st., 3 d.c. around same, fasten in 1st st. of chain of 5 of last row.

4th row.—5 ch.st., 3 d.c. around next chain of 3 of 3d row, 3 ch.st., 3 d.c. around same, fasten, 6 ch.st., 3 d.c. around next ch. of 3, 3 ch.st., 3 d.c. around same, fasten, 6 ch.st., 3 d.c. around next ch. of 3, 3 ch.st., 3 d.c. around same, fasten, 6 ch.st., 3 d.c. around next ch. of 3, 3 ch.st., 3 d.c. around same; work around next chain of 6, * 2 d.c., 3 ch.st. * Repeat 5 times, stopping before 3 ch.st., fasten by 1 s.c. in last 3d d.c. of 1st row.

5th row.—Turn, * 1 s.c., 3 d.c., 1 s.c. around chain of 3. * Repeat 4 times; 3 ch.st., 3 d.c. around next ch. of 3 of last row, * 3 ch.st., 3 d.c. around same, fasten, 6 ch.st., 3 d.c. around next chain of 3 *, repeat to the end of the row. Finally, make 5 ch.st. instead of 3.

Begin again from 2d row.

For the heading, fasten the twine to end of work, then crochet 1 s.c. in every stitch of the edge.

The second row of heading is worked as follows:

Turn, * 3 d.c. in next s.c. of last row, miss next s.c., fasten in following s.c., miss 1, * repeat to end of the row.

[31]

## HAMMOCK.

The tools for making a hammock are—first, a “seine needle,” which may be obtained at any fishing-tackle store, and, second, what is called a mesh board. The needle is made of hard wood and of the shape represented in illustration. The mesh board is simply a piece of common wood about 6 inches long by 2 or 2½ inches wide, according to the size of the mesh desired, and bevelled on one side, being one-half the stretched measure of the mesh. Having provided yourself with the tools as above, proceed as follows:

Take a piece of twine a foot or so long and tie the ends together, making a loop on which to knit the first row of meshes, and hang it on a hook or nail; then fill your needle by tying the end of the twine to the pin in the middle of the needle, and carrying it around the notch and back to the pin until the needle is full, being careful to turn the needle over every time, so that both sides will be alike.

Tie the loose end of twine on the needle to the loop mentioned above, and place the mesh board underneath close to the loop; then carry the needle down under the board and up through the loop, drawing the twine tight; place the thumb (the mesh board being held in the left hand) so as to hold the[32] twine in position on the edge of the mesh board, and throw the bight (or slack) of the twine loosely towards the left, and carry the needle under the right side of the loop and up on the left side through the bight, and pull it down snugly.

The same operation should be repeated, with the exception of putting the needle between the loop and the bight, as it must be carried through the loop and the bight at the same time. In order to make the knot more secure, it would be well to throw the bight again to the left, and bring the needle up through the loop a second time, thus making the knot double. This suggestion applies to the first row of meshes only.

Continue this until you have a sufficient number of meshes for the width of the hammock, 30 being the usual number; then slip the meshes off the mesh board and allow them to hang from the twine on the needle; then place the mesh board underneath, in the same manner as at first, and repeat the original operation, putting the needle through the first mesh instead of the loop, as in the first instance, and making the knot as before. (See illustration.) Follow the meshes along in the same way, until the hammock is the desired length. It is usual to make it about six feet long when stretched for a full-sized hammock, and then to put on each end strings about two feet long, reaching from each end mesh to an iron ring about an inch and a half in diameter, to which the ropes for swinging it are to be attached. These strings can be put on in the same manner as the meshes are knit by simply substituting a piece of board about 2 feet long and 3 or 4 inches wide for the mesh board and using it lengthwise.

TRANSCRIBER’S NOTE
Obvious typographical errors and punctuation errors have been corrected after careful comparison with other occurrences within the text and consultation of external sources.
Except for those changes noted below, all misspellings in the text, and inconsistent or archaic usage, have been retained.
The “Double Double Crochet” stitch abbreviated as “d. d. c.” and referenced on Page 5’s “DESCRIPTION OF TERMS USED IN CROCHET” is not used in any pattern. The Half Double Crochet is referenced as “h.d.c.” on page 9 but not described here. A Half Double Crochet would be described using language from this book as “Turn the twine around the needle once, pass the hook through a loop of preceding row, bring twine through, throw the twine around the needle and draw it through three loops.”
Stitch abbreviations split across lines have been joined to improve legibility.
Page 4. “labrequins” replaced by “lambrequins”.
Page 22. “3 3 ch” replaced by “3; 3 ch”.
*** END OF THE PROJECT GUTENBERG EBOOK TWINE CROCHET WORK, WITH ILLUSTRATIONS ***
Updated editions will replace the previous one—the old editions will be renamed.
Creating the works from print editions not protected by U.S. copyright law means that no one owns a United States copyright in these works, so the Foundation (and you!) can copy and distribute it in the United States without permission and without paying copyright royalties. Special rules, set forth in the General Terms of Use part of this license, apply to copying and distributing Project Gutenberg™ electronic works to protect the PROJECT GUTENBERG™ concept and trademark. Project Gutenberg is a registered trademark, and may not be used if you charge for an eBook, except by following the terms of the trademark license, including paying royalties for use of the Project Gutenberg trademark. If you do not charge anything for copies of this eBook, complying with the trademark license is very easy. You may use this eBook for nearly any purpose such as creation of derivative works, reports, performances and research. Project Gutenberg eBooks may be modified and printed and given away—you may do practically ANYTHING in the United States with eBooks not protected by U.S. copyright law. Redistribution is subject to the trademark license, especially commercial redistribution.
START: FULL LICENSE

## THE FULL PROJECT GUTENBERG™ LICENSE

PLEASE READ THIS BEFORE YOU DISTRIBUTE OR USE THIS WORK
To protect the Project Gutenberg™ mission of promoting the free distribution of electronic works, by using or distributing this work (or any other work associated in any way with the phrase “Project Gutenberg”), you agree to comply with all the terms of the Full Project Gutenberg License available with this file or online at www.gutenberg.org/license.
Section 1. General Terms of Use and Redistributing Project Gutenberg electronic works
1.A. By reading or using any part of this Project Gutenberg electronic work, you indicate that you have read, understand, agree to and accept all the terms of this license and intellectual property (trademark/copyright) agreement. If you do not agree to abide by all the terms of this agreement, you must cease using and return or destroy all copies of Project Gutenberg electronic works in your possession. If you paid a fee for obtaining a copy of or access to a Project Gutenberg electronic work and you do not agree to be bound by the terms of this agreement, you may obtain a refund from the person or entity to whom you paid the fee as set forth in paragraph 1.E.8.
1.B. “Project Gutenberg” is a registered trademark. It may only be used on or associated in any way with an electronic work by people who agree to be bound by the terms of this agreement. There are a few things that you can do with most Project Gutenberg electronic works even without complying with the full terms of this agreement. See paragraph 1.C below. There are a lot of things you can do with Project Gutenberg electronic works if you follow the terms of this agreement and help preserve free future access to Project Gutenberg electronic works. See paragraph 1.E below.
1.C. The Project Gutenberg Literary Archive Foundation (“the Foundation” or PGLAF), owns a compilation copyright in the collection of Project Gutenberg electronic works. Nearly all the individual works in the collection are in the public domain in the United States. If an individual work is unprotected by copyright law in the United States and you are located in the United States, we do not claim a right to prevent you from copying, distributing, performing, displaying or creating derivative works based on the work as long as all references to Project Gutenberg are removed. Of course, we hope that you will support the Project Gutenberg mission of promoting free access to electronic works by freely sharing Project Gutenberg works in compliance with the terms of this agreement for keeping the Project Gutenberg name associated with the work. You can easily comply with the terms of this agreement by keeping this work in the same format with its attached full Project Gutenberg License when you share it without charge with others.
1.D. The copyright laws of the place where you are located also govern what you can do with this work. Copyright laws in most countries are in a constant state of change. If you are outside the United States, check the laws of your country in addition to the terms of this agreement before downloading, copying, displaying, performing, distributing or creating derivative works based on this work or any other Project Gutenberg work. The Foundation makes no representations concerning the copyright status of any work in any country other than the United States.
1.E. Unless you have removed all references to Project Gutenberg:
1.E.1. The following sentence, with active links to, or other immediate access to, the full Project Gutenberg License must appear prominently whenever any copy of a Project Gutenberg work (any work on which the phrase “Project Gutenberg” appears, or with which the phrase “Project Gutenberg” is associated) is accessed, displayed, performed, viewed, copied or distributed:

> This eBook is for the use of anyone anywhere in the United States and most other parts of the world at no cost and with almost no restrictions whatsoever. You may copy it, give it away or re-use it under the terms of the Project Gutenberg™ License included with this eBook or online at www.gutenberg.org. If you are not located in the United States, you will have to check the laws of the country where you are located before using this eBook.

1.E.2. If an individual Project Gutenberg electronic work is derived from texts not protected by U.S. copyright law (does not contain a notice indicating that it is posted with permission of the copyright holder), the work can be copied and distributed to anyone in the United States without paying any fees or charges. If you are redistributing or providing access to a work with the phrase “Project Gutenberg” associated with or appearing on the work, you must comply either with the requirements of paragraphs 1.E.1 through 1.E.7 or obtain permission for the use of the work and the Project Gutenberg trademark as set forth in paragraphs 1.E.8 or 1.E.9.
1.E.3. If an individual Project Gutenberg electronic work is posted with the permission of the copyright holder, your use and distribution must comply with both paragraphs 1.E.1 through 1.E.7 and any additional terms imposed by the copyright holder. Additional terms will be linked to the Project Gutenberg License for all works posted with the permission of the copyright holder found at the beginning of this work.
1.E.4. Do not unlink or detach or remove the full Project Gutenberg License terms from this work, or any files containing a part of this work or any other work associated with Project Gutenberg.
1.E.5. Do not copy, display, perform, distribute or redistribute this electronic work, or any part of this electronic work, without prominently displaying the sentence set forth in paragraph 1.E.1 with active links or immediate access to the full terms of the Project Gutenberg License.
1.E.6. You may convert to and distribute this work in any binary, compressed, marked up, nonproprietary or proprietary form, including any word processing or hypertext form. However, if you provide access to or distribute copies of a Project Gutenberg work in a format other than “Plain Vanilla ASCII” or other format used in the official version posted on the official Project Gutenberg website (www.gutenberg.org), you must, at no additional cost, fee or expense to the user, provide a copy, a means of exporting a copy, or a means of obtaining a copy upon request, of the work in its original “Plain Vanilla ASCII” or other form. Any alternate format must include the full Project Gutenberg License as specified in paragraph 1.E.1.
1.E.7. Do not charge a fee for access to, viewing, displaying, performing, copying or distributing any Project Gutenberg works unless you comply with paragraph 1.E.8 or 1.E.9.
1.E.8. You may charge a reasonable fee for copies of or providing access to or distributing Project Gutenberg electronic works provided that:

- • You pay a royalty fee of 20% of the gross profits you derive from the use of Project Gutenberg works calculated using the method you already use to calculate your applicable taxes. The fee is owed to the owner of the Project Gutenberg trademark, but he has agreed to donate royalties under this paragraph to the Project Gutenberg Literary Archive Foundation. Royalty payments must be paid within 60 days following each date on which you prepare (or are legally required to prepare) your periodic tax returns. Royalty payments should be clearly marked as such and sent to the Project Gutenberg Literary Archive Foundation at the address specified in Section 4, “Information about donations to the Project Gutenberg Literary Archive Foundation.”
- • You provide a full refund of any money paid by a user who notifies you in writing (or by e-mail) within 30 days of receipt that s/he does not agree to the terms of the full Project Gutenberg™ License. You must require such a user to return or destroy all copies of the works possessed in a physical medium and discontinue all use of and all access to other copies of Project Gutenberg™ works.
- • You provide, in accordance with paragraph 1.F.3, a full refund of any money paid for a work or a replacement copy, if a defect in the electronic work is discovered and reported to you within 90 days of receipt of the work.
- • You comply with all other terms of this agreement for free distribution of Project Gutenberg™ works.

1.E.9. If you wish to charge a fee or distribute a Project Gutenberg™ electronic work or group of works on different terms than are set forth in this agreement, you must obtain permission in writing from the Project Gutenberg Literary Archive Foundation, the manager of the Project Gutenberg™ trademark. Contact the Foundation as set forth in Section 3 below.
1.F.
1.F.1. Project Gutenberg volunteers and employees expend considerable effort to identify, do copyright research on, transcribe and proofread works not protected by U.S. copyright law in creating the Project Gutenberg™ collection. Despite these efforts, Project Gutenberg™ electronic works, and the medium on which they may be stored, may contain “Defects,” such as, but not limited to, incomplete, inaccurate or corrupt data, transcription errors, a copyright or other intellectual property infringement, a defective or damaged disk or other medium, a computer virus, or computer codes that damage or cannot be read by your equipment.
1.F.2. LIMITED WARRANTY, DISCLAIMER OF DAMAGES - Except for the “Right of Replacement or Refund” described in paragraph 1.F.3, the Project Gutenberg Literary Archive Foundation, the owner of the Project Gutenberg™ trademark, and any other party distributing a Project Gutenberg™ electronic work under this agreement, disclaim all liability to you for damages, costs and expenses, including legal fees. YOU AGREE THAT YOU HAVE NO REMEDIES FOR NEGLIGENCE, STRICT LIABILITY, BREACH OF WARRANTY OR BREACH OF CONTRACT EXCEPT THOSE PROVIDED IN PARAGRAPH 1.F.3. YOU AGREE THAT THE FOUNDATION, THE TRADEMARK OWNER, AND ANY DISTRIBUTOR UNDER THIS AGREEMENT WILL NOT BE LIABLE TO YOU FOR ACTUAL, DIRECT, INDIRECT, CONSEQUENTIAL, PUNITIVE OR INCIDENTAL DAMAGES EVEN IF YOU GIVE NOTICE OF THE POSSIBILITY OF SUCH DAMAGE.
1.F.3. LIMITED RIGHT OF REPLACEMENT OR REFUND - If you discover a defect in this electronic work within 90 days of receiving it, you can receive a refund of the money (if any) you paid for it by sending a written explanation to the person you received the work from. If you received the work on a physical medium, you must return the medium with your written explanation. The person or entity that provided you with the defective work may elect to provide a replacement copy in lieu of a refund. If you received the work electronically, the person or entity providing it to you may choose to give you a second opportunity to receive the work electronically in lieu of a refund. If the second copy is also defective, you may demand a refund in writing without further opportunities to fix the problem.
1.F.4. Except for the limited right of replacement or refund set forth in paragraph 1.F.3, this work is provided to you ‘AS-IS’, WITH NO OTHER WARRANTIES OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO WARRANTIES OF MERCHANTABILITY OR FITNESS FOR ANY PURPOSE.
1.F.5. Some states do not allow disclaimers of certain implied warranties or the exclusion or limitation of certain types of damages. If any disclaimer or limitation set forth in this agreement violates the law of the state applicable to this agreement, the agreement shall be interpreted to make the maximum disclaimer or limitation permitted by the applicable state law. The invalidity or unenforceability of any provision of this agreement shall not void the remaining provisions.
1.F.6. INDEMNITY - You agree to indemnify and hold the Foundation, the trademark owner, any agent or employee of the Foundation, anyone providing copies of Project Gutenberg™ electronic works in accordance with this agreement, and any volunteers associated with the production, promotion and distribution of Project Gutenberg™ electronic works, harmless from all liability, costs and expenses, including legal fees, that arise directly or indirectly from any of the following which you do or cause to occur: (a) distribution of this or any Project Gutenberg work, (b) alteration, modification, or additions or deletions to any Project Gutenberg work, and (c) any Defect you cause.
Section 2. Information about the Mission of Project Gutenberg
Project Gutenberg is synonymous with the free distribution of electronic works in formats readable by the widest variety of computers including obsolete, old, middle-aged and new computers. It exists because of the efforts of hundreds of volunteers and donations from people in all walks of life.
Volunteers and financial support to provide volunteers with the assistance they need are critical to reaching Project Gutenberg’s goals and ensuring that the Project Gutenberg collection will remain freely available for generations to come. In 2001, the Project Gutenberg Literary Archive Foundation was created to provide a secure and permanent future for Project Gutenberg and future generations. To learn more about the Project Gutenberg Literary Archive Foundation and how your efforts and donations can help, see Sections 3 and 4 and the Foundation information page at www.gutenberg.org.
Section 3. Information about the Project Gutenberg Literary Archive Foundation
The Project Gutenberg Literary Archive Foundation is a non-profit 501(c)(3) educational corporation organized under the laws of the state of Mississippi and granted tax exempt status by the Internal Revenue Service. The Foundation’s EIN or federal tax identification number is 64-6221541. Contributions to the Project Gutenberg Literary Archive Foundation are tax deductible to the full extent permitted by U.S. federal laws and your state’s laws.
The Foundation’s business office is located at 41 Watchung Plaza #516, Montclair NJ 07042, USA, +1 (862) 621-9288. Email contact links and up to date contact information can be found at the Foundation’s website and official page at www.gutenberg.org/contact
Section 4. Information about Donations to the Project Gutenberg Literary Archive Foundation
Project Gutenberg™ depends upon and cannot survive without widespread public support and donations to carry out its mission of increasing the number of public domain and licensed works that can be freely distributed in machine-readable form accessible by the widest array of equipment including outdated equipment. Many small donations ($1 to $5,000) are particularly important to maintaining tax exempt status with the IRS.
The Foundation is committed to complying with the laws regulating charities and charitable donations in all 50 states of the United States. Compliance requirements are not uniform and it takes a considerable effort, much paperwork and many fees to meet and keep up with these requirements. We do not solicit donations in locations where we have not received written confirmation of compliance. To SEND DONATIONS or determine the status of compliance for any particular state visit www.gutenberg.org/donate.
While we cannot and do not solicit contributions from states where we have not met the solicitation requirements, we know of no prohibition against accepting unsolicited donations from donors in such states who approach us with offers to donate.
International donations are gratefully accepted, but we cannot make any statements concerning tax treatment of donations received from outside the United States. U.S. laws alone swamp our small staff.
Please check the Project Gutenberg web pages for current donation methods and addresses. Donations are accepted in a number of other ways including checks, online payments and credit card donations. To donate, please visit: www.gutenberg.org/donate.
Section 5. General Information About Project Gutenberg electronic works
Professor Michael S. Hart was the originator of the Project Gutenberg concept of a library of electronic works that could be freely shared with anyone. For forty years, he produced and distributed Project Gutenberg eBooks with only a loose network of volunteer support.
Project Gutenberg eBooks are often created from several printed editions, all of which are confirmed as not protected by copyright in the U.S. unless a copyright notice is included. Thus, we do not necessarily keep eBooks in compliance with any particular paper edition.
Most people start at our website which has the main PG search facility: www.gutenberg.org.
This website includes information about Project Gutenberg, including how to make donations to the Project Gutenberg Literary Archive Foundation, how to help produce our new eBooks, and how to subscribe to our email newsletter to hear about new eBooks.