## The Project Gutenberg eBook of English Church Architecture of the Middle Ages: An Elementary Handbook

This ebook is for the use of anyone anywhere in the United States and most other parts of the world at no cost and with almost no restrictions whatsoever. You may copy it, give it away or re-use it under the terms of the Project Gutenberg License included with this ebook or online at www.gutenberg.org. If you are not located in the United States, you will have to check the laws of the country where you are located before using this eBook.

Title: English Church Architecture of the Middle Ages: An Elementary Handbook

Author: A. Freeman Smith

Release date: January 20, 2019 [eBook #58736]
Most recently updated: January 24, 2021

Language: English

Credits: Produced by Chuck Greif and the Online Distributed
Proofreading Team at http://www.pgdp.net (This file was
produced from images available at The Internet Archive)

*** START OF THE PROJECT GUTENBERG EBOOK ENGLISH CHURCH ARCHITECTURE OF THE MIDDLE AGES: AN ELEMENTARY HANDBOOK ***

List of Illustrations (In certain versions of this etext [in certain browsers] clicking on the image will bring up a larger version.) Chronology Index: A, B, C, D, E, F, H, I, J, L, M, N, O, P, Q, R, S, T, V, W. (etext transcriber's note)

{i}

{ii}

ENGLISH CHURCH ARCHITECTURE OF THE MIDDLE AGES
ENGLISH CATHEDRALS

CANTERBURY—PETERBOROUGH—
DURHAM—SALISBURY—LICHFIELD—
LINCOLN—ELY—WELLS—WINCHESTER—
GLOUCESTER—YORK—LONDON
By Mrs. S. van Rensselaer. Illustrated
with one hundred and fifty-four Drawings
by Joseph Pennell. Also with Plans
and Diagrams. Fifth Edition, revised and
corrected. Cloth, 20s. net

HANDBOOK OF ENGLISH CATHEDRALS
By Mrs. S. van Rensselaer. Illustrated
with Drawings by Joseph Pennell. Also
with Plans and Diagrams. Cloth, 10s. 6d. net

T. FISHER UNWIN, LTD., LONDON

{iii}

ENGLISH CHURCH
ARCHITECTURE
OF THE MIDDLE AGES
AN ELEMENTARY HANDBOOK
By A. FREEMAN SMITH

For many years Art Master and Instructor in all Architectural Subjects
in the Municipal School of Art, Birmingham
WITH TWELVE PLATES
T. FISHER UNWIN, LTD.
LONDON: ADELPHI TERRACE
{iv}
First published in 1922.

{v}

[All Rights Reserved]

## PREFACE

THE object of this little work is to give an outline of the leading characteristics of Gothic Architecture, as found in churches of the Middle Ages in England. And it is hoped that it may be found useful to those visiting those noble buildings, whose antiquity and inseparable connection with the history of the country in their growth and development, in addition to the highest purpose for which they were erected by the faithful followers of the Founder of the Christian Faith, entitle them to veneration and careful study in the realms of history, art, and religion.

Its purpose as a handbook is to explain the origin and use of some of the forms which are presented to the eye of the visitor to these ancient monuments, not as being the result of caprice, or mere æsthetic motives, {vi}but as derived originally from a deep conviction of the living truth which their founders professed, and which they attempted to express in all their constructive work.

It is intended that the book may also be found useful as an elementary introduction to the study of Gothic Architecture through the many elaborate and exhaustive treatises which are published on the subject. To such students, literary study should be supplemented by personal acquaintance with buildings recognised as standards of excellence.

The Introduction deals with symbols as the motive of Gothic design. In the following pages the various periods of English Gothic are defined by their predominating forms and ornaments dating from the seventh to the sixteenth centuries. Simple examples have been chosen in order to avoid the confusion which might result from the choice of more complex illustrations.

In the preparation of the illustrations the works of Agincourt, Didron, {vii}Owen Jones, and the late Jethro A. Cossins, have been consulted for those of Plate I. Of the remaining, Plate II., Fig. 5, and Plate V., Fig. 1, are from works of Parker and Rickman respectively. Five details are from photographs; the remainder are from original sketches and studies by the Author.{ix}{viii}

## LIST OF PLATES

PLATE |  | PAGE
I. | Byzantine and Early Christian | 13
II. | Anglo-Saxon | 21
III. | Norman | 27
IV. | Transitional, 1145-1190 (Norman to Early English) | 35
V. | Early English | 39
VI. | Decorated | 45
VII. | Decorated | 47
VIII. | Perpendicular | 53
IX. | Perpendicular | 55
X. | English Gothic Roofs | 63
XI. | Vaulting | 71
XII. | Vaulting | 73

{x}

{xi}

## CHRONOLOGY

The popular classification of English Gothic Architecture divides the style into four periods, thus:

Norman | William | I., | 1066, | to Richard | I., | 1189.
Early English | Richard | I., | 1189, | to Edward | I., | 1272.
Decorated | Edward | I., | 1272, | to Richard | II., | 1377.
Perpendicular | Richard | II., | 1377, | to Edward | VI., | 1547.

These terms are useful, but not sufficiently descriptive. They were superseded by the late Edmund Sharpe’s “Seven Periods,” the terms of which are derived from the forms of the windows and their tracery, but are applicable to other details.

SHARPE’S “SEVEN PERIODS.”

Saxon |  |  | 1066.
Norman | 1066 | to | 1145.
Transitional | 1145 | ” | 1190.
Lancet | 1190 | ” | 1245.
Geometrical | 1245 | ” | 1315.
Curvilinear | 1315 | ” | 1360.
Rectilinear | 1360 | ” | 1550.

{xii}

{13}

## PLATE I

BYZANTINE AND EARLY CHRISTIAN{14}

{15}

PLATE I

# English Church Architecture
of the Middle Ages

## INTRODUCTION

Plate I

BYZANTINE AND EARLY CHRISTIAN

THE term Gothic was applied originally as one of contempt in the fifteenth century by the architects of the Renaissance, who attempted to reproduce the ancient architecture of Rome, and considered Mediæval Art, which had ruled all departments of design throughout Europe during the three preceding centuries, to be no better than the invention of the Barbarians, the Goths, and the Vandals, who overran the Roman Empire in the fourth century. During the three previous centuries the persecuted converts to Christianity were driven to take refuge in any hiding-place available. In Rome they descended to the Catacombs, the underground workings of the ancient Roman stone quarries, consisting of narrow,{16} low passages, their aggregate lengths amounting to hundreds of miles. There they quarried out of the rock their chambers for assembly, where they gathered for worship in the light of torches or lamps, and excavated recesses for the burial of their dead. These chambers were imitated in the form of the Crypts (hidden chambers) existing under some churches and cathedrals. (Compare Plate I., Figs. 1 and 2.) The walls of the catacombs have rude incised inscriptions and carvings revealing the Christian Faith by symbols, such as the cross, suggesting the Crucifixion—the emblem of sacrifice; the circle, the line without end, the symbol of Eternity (Plate I., Fig. 3); the triangle, trefoil, and triquetra, symbols of the Trinity (Figs. 6, 7, and 8); the quatrefoil of the four evangelists (Figs. 9 and 10). The fish was adopted as a symbol of the Redeemer, because the letters of the Greek word icthys, when used as an acrostic, gave the initials of the words—Jesus, Christ, God, Son, Saviour (Plate I., Fig. 11). This symbol was extensively adopted in the decoration of baptismal fonts.

The Vesica piscis (Latin, the bladder of a fish) (Plate I., Fig. 5) was used as a nimbus or{17} glory to surround the figure of a sacred personage in sculpture and in painting. Its name shows the use of Latin terms in the Roman Church as distinguished from the Greek in Byzantium, which was an ancient Greek city adopted by Constantine, the Christian Emperor, as the capital of the eastern division of the Roman Empire under the new name of Constantinopolis—the modern Constantinople. But the term “Byzantine” has been retained in matters relating to art. Plate I., Figs. 15 and 16, show the Greek Cross, which is a version of the Greek letter chi combined with the letter rho (similar to the English P). This symbol represented the name Christ, and was the Christian standard, the Labarum, chosen by the Emperor Constantine.

Plate I., 3A. The sacred monogram generally found in church decoration stands for the Latin phrase Jesus hominum Salvator—“Jesus, the Saviour of men.” The Greek letters IHS (iota, eta, sigma) gave the first three letters of the name Jesus.

In the plan of an English cathedral or cruciform church, the symbol of the Latin Cross is made the basis of its form (Plate XI., Fig. 1).{18} (The Byzantine or Greek Cross has the four limbs of equal length.) The Nave, N. (Latin, navis, a ship, a symbol of the Church), is built from west to east. The Choir or Chancel, which is screened off by a Cancellum or lattice, is in continuation of the Nave to the east end. This in some cathedrals includes the Lady Chapel, which was in mediæval times dedicated to the Virgin Mary.

In several churches and some cathedrals the head of the Cross, the Chancel or Choir, is not in line with the Nave, but is slightly inclined to one side—not in all cases the same side. Two explanations are given for this, one being its orientation—i.e., the axis of its length points to the rising of the sun on the day of its foundation, which does not coincide with that of the Nave, the Chancel having been commenced at an earlier or later date and different season of the year. The other theory is that it symbolises the head of Christ falling on one side in death.

Plate I., Fig. 14 (from the “Grammar of Ornament”), shows an ornamental design composed entirely of early Christian symbols. Plate I., Figs. 12 and 13, carved ornament and{19} a capital bearing crude resemblance to an ancient Ionic capital. Both Figs. 12 and 13 are under the influence of Greek and Roman Art without reference to symbolism.

Plate I., Fig. 4, shows a chevron (a French military ornament), a decoration dating back to ancient Egypt, where it symbolised the waves of the Nile, and was adopted in many later periods, and became conspicuous in the Norman arches of English architecture.{21}{20}

## PLATE II

ANGLO-SAXON

{22}

PLATE II

{23}

## Plate II

ANGLO-SAXON

THERE can be no doubt that Christianity found its way into Britain early during the Roman occupation, but was suppressed through the violent persecutions by the Pagan tribes who ruled following the Roman departure A.D. 410, to be revived and further developed after the mission of St. Augustine, A.D. 597, from Rome to the Anglo-Saxons, who occupied Britain between the fifth and eleventh centuries.

The church of Greenstead, in Essex, is one of the most ancient in the country, and was built by Anglo-Saxons. Its walls are of substantial logs of timber placed upright upon a foundation of rude stonework. This method appears to be a survival of their method of building their dwellings.

Of stone buildings, the church tower of Barton-on-Humber (Plate II., Fig. 6) is a good example of Anglo-Saxon work. In it the ex{24}ternal angles of the tower and of the door and window openings have their quoins (corner stones) of “long-and-short” work, the name applied to Saxon masonry of this kind, in which long stones are placed on end with short stones laid flat, suggesting their origin to be the work of carpenters who would place timbers in such positions, contrasted with that of masons, who would place all stones horizontally or at right-angles to pressure.

In this example and the very fine one at Earls Barton, Northamptonshire, this “long-and-short” work is carried over the exterior of the wall as a kind of surface decoration.

Plate II., Fig. 3, shows the present-day manner of framing timbers in a partition with sill (s.), posts or studs (p.), lintel (l.), inclined struts, and corbel-blocks (c.b.).

Saxon timber framing would be on similar lines, and this manner was perpetuated traditionally in their stone walls. The practice of imitating woodwork in stone and vice versa is one to be found in the works of all ages from remote antiquity. The heads of Saxon door and window openings were either semicircular (Plate II., Figs. 7, 8, and 9) or formed by placing{25} two stones inclined to each other thus—ʌ, and a short column or rude baluster was sometimes placed between two windows.

[Note.—The window over the clock face (Plate II., Fig. 6) is an insertion of a later period.]

The interesting little church at Bradford-on-Avon, Wiltshire, shows the same manner of building (Plate II., Fig. 1).

Anglo-Saxon bell-towers appear to have been generally covered with a roof of the form shown in Plate II., Fig. 5, as at Sompting, Sussex.{27}{26}

## PLATE III

NORMAN, 1066-1189

{28}

PLATE III

PLATE III

{29}

## Plate III

NORMAN, 1066-1189

THE Norman period dates from A.D. 1066, though the Norman manner of building had been adopted after the year 1000, when church building was revived after suspension in anticipation of the Millennium, which was expected to bring the end of the world. That dreaded year having safely passed, church building was vigorously revived. Timber construction had led to frequent disaster by fire, and as larger buildings were now required, better construction became imperative. Masonry must supersede carpentry in wall construction, and the necessary skilled labour came from Normandy.

The influx of superior talent following the Norman Conquest resulted in great improvement in every department of building. Stately cathedrals were founded, each for the reception of the cathedra or throne of the bishop. Abbeys{30} and monasteries and parish churches for the clergy were built throughout the land, as proved by the existence of Norman work in most parts of the country.

Every period of English Gothic architecture has certain forms appearing in the general composition and details which help to fix the period to which they belong. In the Norman the square and the circle, the right angle and the semicircle, are the prevailing figures suggestive of strength and severity so evident in the impressive naves of Ely, Peterborough, Norwich, Gloucester, Tewkesbury, and the fortress-like cathedral of Durham.

Plate III. gives a few details of work of the Norman period. The term pier (Plate III., Fig. 1) defines the pillars or masses of masonry supporting the arches between the nave and aisles of a church. This example (Plate III., Fig. 1), from St. John’s Chapel in the White Tower of London, William the Conqueror’s residence, is circular with a square capital chamfered down to the circular pier, and has a slightly moulded abacus (the crowning moulding of a capital).

Plate III., Fig. 2, the cushion capital, is the{31} simplest kind of Norman capital. It is cubical, with its square faces rounded down to the shaft.

[Note.—The shafts of all English Gothic columns are cylindrical—i.e., without any diminution towards the top, in contrast with Greek and Roman shafts, which are always diminished.]

Plate III., Fig. 3, is the capital of a respond—a half-column attached to a wall and carrying an arch or part of a roof.

Plate III., Fig. 4, the corbel-table, or cornice underneath the eaves of a roof (corbel—a bracket).

Plate III., Fig. 5, the base of a pier with spur ornaments.

Plate III., Fig. 6, fragment of a Norman arch of four orders, each order being a separate arch, three of which are enriched with the Norman chevron. The dripstone or hood-moulding (d.s.) encloses the arch as in Plate III., Fig. 8, though its original function—to protect the moulding under it from weather—is not needed here, but it is generally introduced to give effective finish to the arch. The capitals in this group are scallop capitals. A small portion{32} of a similar capital is shown at the right hand of Plate III., Fig. 3.

Plate III., Fig. 7, is a Norman font of the simple bowl form enriched with carved Norman heads connected by Byzantine ornament and surrounded with a Norman arcade of intersecting arches—a feature often introduced in the walls of churches and cathedrals.

Plate III., Fig. 8, is a double-recessed window with an arch of three orders. The columns in the positions shown are called jamb-shafts or nook-shafts; those on the right are detached and may be removed, leaving the bases and capitals remaining. On the left the shafts are engaged—i.e., form part of the masonry of the wall. These two varieties are never found together as here, but are thus shown for convenience. The capitals are a variety of the cushion capital.

Plate III., Fig. 9, is a cushion capital with the triquetra symbol of the Trinity (Plate I., Fig. 8).

Byzantine influence is evident in the ornament of the capitals (Plate III., Figs. 1, 3, and 9), in the chevron (Plate III., Fig. 6), and the decoration of the font (Plate III., Fig. 7).{33}

Norman walls depended for their strength upon their thickness, with the slight addition at intervals, where lateral pressure occurred, of thin pilaster-like buttresses projecting only a few inches equally from bottom to top.{35}{34}

## PLATE IV

TRANSITIONAL, 1145-1190

(NORMAN TO EARLY ENGLISH)

{36}

PLATE IV

{37}

## Plate IV

TRANSITIONAL, 1145-1190

THE period of Transition from Norman to Early English dates from 1145 to 1190, in the reigns of Stephen and Richard I., the period when architecture gradually passed from the massiveness and severity of Romanesque, as expressed in the Norman, to the delicate refinement of Early English Gothic. In its general character there is much that is common to both periods. It is easily distinguished in its details as capitals, arches, carving, etc.

Plate IV., Figs. 1 and 3, show Transitional capitals in which the square abacus of the Norman remains and the concave surface of the body or bell contrasts with the convex of the Norman (Plate III., Figs. 2, 3, 6, and 9). Rude carving suggestive of foliage was sometimes introduced. The placing of two pointed arches under a semicircle (Plate IV., Fig. 2) is especially indicative of the Transitional period.{38}

In the Transitional period the pointed or Gothic arch was first introduced, and established as the most characteristic feature of the Gothic style on account of its superior strength and fitness. In the Transition, hollows were introduced separating the rounds in mouldings (Plate IV., Fig. 4). In other respects Transitional work differs little from Norman.{39}

## PLATE V

EARLY ENGLISH
LANCET, 1190-1245
GEOMETRICAL, 1245-1315
{40}

PLATE V

{41}

## Plate V

EARLY ENGLISH, 1189-1272

IN the Early English period knowledge of the true principles of architectural design and construction advanced considerably—mouldings and carving attained the highest refinement, and the work of the Early English period is admitted to be the purest of the Gothic style.

Improved scientific construction is most evident in the walls. The development of stone-vaulted roofs (a protection against fire) carried by arched ribs brought down the incumbent load on to the walls, producing thrusts upon them which had to be provided against. The old manner of making the wall of great thickness was wasteful and unsatisfactory. The happy idea of the Gothic buttress fulfilled all the requirements, and produced one of the most beautiful features of the Gothic style. It was built in diminishing stages, its outline enclosing the graceful parabolic curve of nature{42}—the path of the combined thrusts and their opposing reactions. This structure was carried to perfection when combined with the flying-buttress (Plate VII., Fig. 10), which conducted the thrust from the lofty wall of the nave over the external roof of the aisle by an arch on the wall-buttress, which was strengthened to do its work by the addition of a heavy pinnacle. Plate V., Fig. 9, from Lichfield Cathedral, shows two buttresses of the Lancet period built to meet the thrust of the ribs carrying the vaulting of the Chapter-house and Library over. In one of these the approximate direction of the thrusts is indicated by the arrows a, b, which, if unopposed, would cause a collapse; the ultimate deflection of their path by the weight of the superincumbent masonry is indicated by dotted lines within the buttress, thereby producing equilibrium through the opposing resistance from the foundations along the same path.

In Plate V., Figs. 10 and 11, the piers had columns surrounding them whose shafts in the Lancet period were detached, but connected at their extremities by moulded stone bands (A, B), and at the bases and capitals. These{43} piers were sometimes carried to a great height, as those in Westminster Abbey, which have three of these stone bands in their height. In the Geometrical period the shafts formed part of the main pier, were not detached, and resembled mouldings (Plate V., Fig. 11). Such shafts were described as engaged.

Plate V., Fig. 7, shows a tower with a broach-spire belonging to the Early English period. In the figure the four broaches are the small pyramids covering the squinch arches or squinch corbels, which carried four of the eight sides of the octagonal spire across the angles of the tower.

Plate V., Fig. 4, shows three Lancet windows under a single arch or dripstone. This grouping of the windows soon suggested the design of tracery windows, in which the lights are separated by mullions, the simplest form being as represented in the Lichfield Chapter-house in Plate V., Fig. 9. Geometrical arrangements were invented from the simple one (Plate V., Fig. 5) to the elaborate windows and arcades of Westminster Abbey. Cusps (spear points) were formed in the tracery, the Soffit-cusp (s.c.) projecting from the underside of the mullion,{44} indicating early work and uncommon. All other cusps were worked on the chamfer (c.c), their points being variously shaped.

In Plate V., Fig. 8, the capitals were either moulded, or carved with stiff-leaf foliage, being conventional—i.e., designed on natural principles, but not in imitation of nature, and sometimes of great beauty, but never so delicate as to suggest its unsuitability to the material in which it was wrought. Hollows in the arch and other mouldings were enriched with the tooth ornament (Plate V., Fig. 12), which occurs in the Lancet period only.

Plate V., Fig. 2, shows the decoration of gables with crockets and finial.

Plate V., Fig. 3, shows diaper ornaments used in wall decoration.

Plate V., Fig. 6, shows a string course and dripstone. All mouldings consist of large rounds and deep hollows, separated by fillets (a, b), and are frequently arranged in extensive groups, as in doorways, arcading, etc.

The Cathedral of Salisbury is the only one which is throughout belonging to the Early English period.{45}

## PLATE VI

DECORATED, 1272-1377
GEOMETRICAL, 1245-1315
CURVILINEAR, 1315-1360
{46}

PLATE VI

{47}

## PLATE VII

DECORATED, 1272-1377

{48}

PLATE VII

{49}

## Plates VI and VII

DECORATED, 1272-1377; GEOMETRICAL, 1245-1315; CURVILINEAR, 1315-1360

THE term “decorated” is applied to the work of this period because of the superfluity of its ornaments. Almost every feature was enriched with carved ornament. The predominating form is the curvilinear line, the ogee or ogival (Plate VI., Fig. 2), Hogarth’s “line of beauty and grace,” which occurs in the lines of tracery, the shape of arches, sections of mouldings, and of foliated ornament.

The Geometrical period, 1245-1315, is the overlapping of Early English and Decorated. The term Geometrical is applied on account of the window tracery, which is made up of circles and triangles more or less elaborate. The change from Geometrical to Curvilinear or flowing tracery is demonstrated in Plate VII., Figs. 1, 2; Plate VII., Fig. 2, being a slight alteration of Plate VII., Fig. 1.{50}

Plate VII., Fig. 5, reticulated—net-like—is a common example produced in the same manner as Plate VII., Fig. 2, and is adaptable to all shapes of windows. Many elaborate and beautiful designs were produced on these principles by extension of such elements as in Plate VII., Fig. 3.

Plate VII., Fig. 4, is a common type of window; an extension of the simple two-light window (Plate V., Fig. 9), frequently enriched with cusps and ball-flower (Plate VI., Fig. 3) in the hollows of the mullions.

In Plate VII., Fig. 10, the buttresses are decorated with niches for statuary. A flying-buttress is shown (F.B.), carrying the thrust of the stone-vaulted roof of the nave over the external roof of the aisle into the main buttress, whose weight and consequent stability are increased by the heavy pinnacle. The smaller buttress (C.) resists the thrust of the window arches. Norwich Cathedral displays an interesting array of flying-buttresses.

Plate VI., Fig. 6, shows a tower and spire at the crossing of nave and transepts. The base of the spire and its broaches (Plate V., Fig. 7) are concealed by a parapet wall, with battle{51}ments protecting a footway round the spire, which could be used as a place of observation. Mouldings in the Geometrical period attained the greatest refinement. Many can be favourably compared with those of the best Greek periods.

Arches continued to be built in square orders (Plate III., Figs. 6 and 8), and consisted of round mouldings, generally separated by deep hollows and fillets (Plate VII., Fig. 7).

In mouldings of the Curvilinear period (Plate VII., Fig. 8) the ogee superseded the round, and the hollows were shallower. Towards the end of the period the square orders ceased, and the planes of the orders were at about 45° with the vertical (Plate VII., Fig. 9; compare with Plate VIII., Fig. 12).

The wave-moulding (Plate VII., Fig. 9) and the scroll-moulding (Plate VII., Figs. 9, 12, and 13), supposed to resemble a parchment scroll, are conspicuous in the Curvilinear. The general character of the ornament is indicated on Plate VII., in most of which the ogee line is apparent.

The ball-flower (Plate VI., Fig. 3) is a dis{52}tinctive feature of the Decorated period superseding the tooth ornament of the Lancet (Plate V., Fig. 12). It was applied to hollow mouldings of arches and tracery of windows, vaulting, and spires.

Capitals were moulded as in the section (Plate VII., Fig. 13), or carved, as Plate VI., Fig. 4, generally in imitation of natural foliage, varying from a bold conventionalism (Plate VI., Fig. 5) to a close imitation of nature, as Plate VI., Fig. 1 (a.a.). Animal forms and small human figures were occasionally introduced. Figure sculpture reached its highest degree of excellence in this period.

Construction was further advanced, but in design the climax had been attained in the Geometrical period, and a very gradual decline set in, as shown in excessive ornamentation and literal imitation of natural forms in stonework, which is unsuitable for such delicate treatment on account of its fragility.

The increasing wealth of the nation during this period is indicated by the grandeur of the buildings and the redundancy of ornament.{53}

## PLATE VIII

PERPENDICULAR, 1377-1547

RECTILINEAR, 1360-1550

{54}

PLATE VIII

{55}

## PLATE IX

PERPENDICULAR

{56}

PLATE IX{57}

## Plates VIII and IX

PERPENDICULAR, 1377-1547

RECTILINEAR, 1360-1550

THE term “perpendicular” was applied to the work of this period, the last of English Gothic, on account of the predominance of vertical lines in the whole architectural design, and especially in window tracery.

A comparison of Plate VII., Fig. 5, net tracery, with Plate IX., Fig. 5, rectilinear, will explain how the latter was developed from the former by extending the sides of the meshes of the net by straight lines into the summit of the window. But as the term perpendicular is only a relative one, not necessarily meaning vertical, the term rectilinear was substituted, being descriptive of the general character of the whole design in mass and detail. In this work, however, the term “perpendicular” is preferred as the one most generally known. Windows became so large, chiefly for the{58} display of stained glass, as to reduce the wall spaces between them to little more than piers, and transoms (horizontal mullions) had to be introduced to strengthen the vertical mullions. [See Plate IX., Figs, 1 and 2 (a.b.), belfry windows in these examples.]

Loftiness is a special trait of the Perpendicular period. Walls were carried to a greater height than previously. The external roof was frequently covered with lead, and inclined at an angle easy to walk upon. The roof-timbers were supported by ornamental principals exposed to view from the interior, or there was a stone-vaulted internal roof of rich design, the increased thrusts upon the walls being counteracted by larger buttresses.

Tall towers were built, such as those of York Minster, Gloucester, Worcester, and the churches of Boston (Lincolnshire), Wrexham, Taunton, and many others of magnificence. Plate IX., Figs. 1 and 3, give varieties of smaller parish church towers. In these the Tudor arch and square-headed window are shown. Spires are not so common as in the preceding periods. Buttresses were placed diagonally at{59} all corners, scientifically the best position (Plate IX., Figs, 1 and 2).

In large churches external wall surfaces were enriched with panelling, covering in some cases the whole from ground to summit, and combined with open tracery in the battlements. In the interior the same kind of decoration prevailed, and in some cases the window tracery was carried below the glass down to the floor as panelling.

Plate IX., Figs. 4A and 4B, gives the comparative shape of battlements.

Arch-mouldings (Plate VIII., Fig. 12) generally included the large hollow also common in the window jambs. The plane of the arch-mouldings was inclined to the vertical 45° (Plate VIII., Fig. 12). The usual dripstone (d.s.) and some of their corbels are shown in Plate VIII., Figs. 1 and 3. Piers (Plate VIII., Fig. 11) were of the simple form shown with columns at the angles, single, or in groups, as Plate VIII., Fig. 13, the general contour of the pier being a rhombus or lozenge in plan.

The ogee arch with crockets and finial was continued from the Decorated period.{60}

The Tudor or four-centred arch (Plate IX., Figs. 1 and 6) belongs to the late Perpendicular period.

Plate VIII., Fig. 4, shows a common form of Tudor door-head with the label or square dripstone and carved spandril (a triangular space). Columns were circular, with octagonal bases and capitals, the latter moulded or carved with oak-leaf foliage or conventional ornament, resembling that in Plate VIII., Fig. 9. Corbels with shields (Plate VIII., Fig. 9), armorial bearings, and the Tudor rose (Plate VIII., Fig. 2), frequently occur.

Many Perpendicular churches are rich in ornamental woodwork: choir stalls with lifting seats (misereres), under which are grotesque carvings; poppy-heads (Fr. poupée, a doll), the bench-end ornaments which sometimes carried a small carved figure among foliage; panelled screens crowned with brattishing (Plate VIII., Fig. 5), and other ornaments. The term brattishing is also applied to the open tracery of some battlements of the Perpendicular period.

The Perpendicular is the longest of the English Gothic periods. In it Gothic con{61}struction attained its climax; ornamentation declined from a refined realism to coarse conventionalism, coinciding with the decline of spiritual life in the Church. Cathedrals and churches increased in all dimensions, and everything showed the tendency towards the renaissance of classic art which was flourishing on the Continent. Classic mouldings were imitated, and carved ornament of pure Italian design was applied to decorate Gothic forms—notable instances being the tomb of Henry VII. in Westminster Abbey, and the Salisbury Chantry in Christchurch Priory near Bournemouth. Both were the work of Torregiano, a contemporary of Michael Angelo.

The English people clung to their Gothic style for a century after the same had almost disappeared from the Continent, and in the Elizabethan period, 1558-1603, classic details, including the five orders, were completely incorporated into Gothic design. The pointed arch disappeared; the Roman semicircle took its place. Brickwork superseded masonry, roof construction was concealed, and all kinds of shams were introduced. Then came a period of close imitation of Greek and Roman temples,{62} until the Gothic revival under its pioneer, A. W. Pugin (b. 1812, d. 1852), whose literary works are very instructive and interesting reading. The present-day (1922) tendency is towards a revival of Byzantine architecture. {63}

## PLATE X

ENGLISH GOTHIC ROOFS

{64}

PLATE X

{65}

## Plate X

ENGLISH GOTHIC ROOFS

NEXT in importance to the construction of substantial walls comes the necessity of weather-proof and storm-proof roofs, such as should preserve the stability of the walls, or their disintegration would be hastened by that which should be their protection.

The nature of the covering and the action of weather are the principal factors affecting their design and construction. The rigours of the English climate require a covering to be such as to prevent the penetration of rain, and their support to be strong enough to resist the pressure of snow and the hurricane. The high-pitched roof (of steep inclination) is common to all periods of English Gothic. The average Norman roof was pitched about 45°, its apex being about a right angle composed agreeably with the semicircular arches in the gables. The higher-pitched roofs came simultaneously with the introduction of the{66} pointed arch, sometimes at a pitch of 60°, ultimately declining to about 20° or less in the late Perpendicular period. The outer covering is generally of boards overlaid with tiles or sheet-lead, the latter being imperative in the low-pitched roofs. The whole of the covering is carried by common rafters or spars rising from the walls to the apex of the roof.

Plate X., Figs. 1 and 2, show two ordinary principals or trusses. These are in no sense Gothic, but are here given to more clearly explain the principles of roof construction. The common rafters (c.r.) bearing the covering are of light timber, tending to bend under the weight; to prevent this purlins (P.), stout beams, are placed at suitable intervals, and these are carried at their ends by the roof trusses. The tie-beam (t.b) is the chief beam of the truss. The principal rafters (p.r.) are framed into it and into the heads of the King and Queen posts. In the Queen-post-truss the collar unites the Queen posts; struts and cross-braces complete the structure. In a properly constructed roof-truss all the stresses are neutralised in the truss itself, and the whole{67} framework rests as a dead weight upon the walls without any lateral thrust to force them out of the vertical. The King-post-truss is suitable to roofs up to 30 feet span, the Queen-post-truss to 40 feet.

Open timber roofs have their construction visible from the interior. Plate X., Fig. 8, shows a crude Queen-post-truss in an old Worcestershire church, in which the tie-beam has been chosen from a bent log so as to prevent its bending under the roof load. In the trusses (Plate X., Figs. 1, 2) the King and Queen posts act like the keystones of an arch, so that by bolting or strapping up with ironwork at points s.s. these posts are put into a state of tension, the tie-beam (t.b.) is pulled up to a camber, or curve, and is also in tension. In the crude Queen-post-truss (Plate X., Fig. 8) these conditions are reversed, for the tie-beam supports the Queen posts. In Plate X., Figs. 1 and 2, all the spaces in these trusses are triangular, a fact which ensures stability where the parts are of proper strength and properly united. Plate X., Fig. 4, is a trussed rafter roof requiring no purlins nor principal—each common rafter is a truss. This kind of roof is suitable{68} only to small spans; its weakest part is from a. to b.

In the roof-truss, or principal, the Gothic architects objected to the tie-beam as an obstruction to the sense of loftiness, so desirable in the church interior, and therefore invented the hammer-beam principal (Plate X., Fig. 7), which resembles a Queen-post-truss, having a collar and King post. The hammer-beams (h.b.) are substitutes for the tie-beam.

In this principal the space between the collar and the apex of the roof is satisfactorily trussed, but from the collar downwards the Queen posts (Q.p.) and wall posts (w.p.) with their braces (b.) become mere brackets supporting the small King-post-truss above, bringing its load as low as possible on to the walls, so that their weight of masonry and buttresses may effectually resist the lateral thrust of the roof upon them.

Plate X., Fig. 5, shows a collar principal with curved braces. The tendency of all roof principals is to spread at the walls; this has been met by modern church-builders by introducing an iron tie-rod in place of a tie-beam, thus forming a triangle, the only form of absolute stability, for the whole of the prin{69}cipal, as indicated by the dotted line connecting the hammer-beams in Plate X., Fig. 7.

Plate X., Fig. 6, shows a low-pitched Perpendicular roof with principals and half-principal. The common rafters are concealed by a panelled ceiling, the panels being formed by principal rafters and purlins. The arched trusses bring part of the thrust low down on to the walls, which are strengthened by heavy buttresses on the outside. The half-principal is placed over a window arch.

Plate X., Fig. 3, shows a low-pitched roof and ceiling supported by a tie-beam only, strengthened at its bearings by wall posts and braces.{71}{70}

## PLATE XI

GOTHIC VAULTS

{72}

PLATE XI

{73}

## PLATE XII

GOTHIC VAULTS

{74}

PLATE XII

{75}

## Plates XI and XII

GOTHIC VAULTS

STONE-VAULTED roofs became necessary in church building early in the Norman period for security against fire. They were made after the Roman manner, semicircular, with similar vaults intersecting at right angles. The lines of their intersections are the groins. When two intersecting vaults are of equal semicircles, each groin is a semi-ellipse. This groin is the weakest part of the vault; in order to strengthen it the Normans built an arch called the groin rib, underneath the groin, to support it. Difficulties were met in forming intersecting vaults of unequal span, clumsy contrivances were resorted to, until, in the Transition period, 1145-1190, the introduction of the pointed arch solved the problem, and led the way to the development of Gothic vaulting. The Roman and Norman vaults were built upon temporary centering. A centre is a timber frame made like a roof-truss shaped{76} to the form of the arch; a series of centres were placed at convenient distances apart and covered with strong boarding upon which the vault was built. After the masonry was completely set, the temporary centering was removed, leaving the vault to carry itself.

As the system of vaulting developed, cross ribs and wall ribs (Plate XI., Fig. 3) were added, and much of the temporary centering was dispensed with; ornamental arrangements were designed by introducing more ribs, and the web—the covering surface of masonry—was reduced to small panels in the Decorated and Perpendicular periods. In the Tudor period, 1485-1558, the web became the principal part, the ribs being mere mouldings worked upon its surface in the form of fan-vaulting, a simple example of which can be studied in the south porch of Chester Cathedral, and the most elaborate in the roof of the Chapel of Henry VII., Westminster Abbey.

A bay of a cathedral is one of the spaces into which its length is divided by the supports of the roof as piers, arches, or principals. The bays of the aisles are usually square—those of{77} the nave, choir, or transepts rectangular on account of their greater width.

Vertically each of the bays of the nave, etc., is divided into three stories (Plate XI., Fig. 2), the groundstory rising from the floor; the triforium, or blindstory, having no windows, is over the aisles, and the clerestory over the triforium. The prefix clere—bright—indicates the brilliancy of its light.

In the Norman period these three divisions were nearly equal in height. In the succeeding periods the groundstory attained about half of the total height of the bay, the clerestory was extended downwards, and the triforium reduced, until, in the Perpendicular period, it entirely disappeared.

Plate XI., Figs. 3 and 4, show a few square bays of Gothic vaulting in skeleton diagrams with the forms of plan indicated by dotted lines upon their base-planes. All the lines represent ribs.

Plate XI., Figs. 2 and 3, show quadripartite vaulting—i.e., having four compartments in one bay. This is the simplest form of Gothic vault, and belongs chiefly to the Early English period. The ribs ah, bh, ci, di are wall ribs;{78} bg, cg, ag, dg, are cross ribs; ae, ce, be, de, are the diagonal ribs. The ridge-ribs eg and h, e, i, are horizontal, and intersect the summits of the cross ribs and diagonals. At every intersection there is generally a carved keystone or boss.

In the vaulting of a nave the breadth across is about twice the breadth of the aisles, so that the nave bays are not square, but rectangular.

Plate XI., Fig. 4, and Plate XII., Fig. 2, show lierne-vaulting, having lierne-ribs, the short ribs joining and supporting all the ascending ribs as h, k, l, m, g.

Plate XII., Figs. 2 and 3, are lierne vaults. That shown in Fig. 3 is under the belfry of a church tower at Coventry, with circular opening for hoisting the bells.

The detail at B shows the method of collecting the three ribs into one at the springers in the corners A, B, C, D, by small arches in the tracery of ribs.

Plate XII., Fig. 1, shows fan-vaulting having no ribs. The lines shown indicate mouldings on the masonry imitating ribs. The structure is built up of slabs of stone, accurately joined{79} together forming concave half-cones, their vertices being the springers of the vault. The dotted lines show some of the jointing; the other lines represent the imitation ribs. The crown of the vault is the flat surface gh, gi, generally richly ornamented.{81}{80}

## INDEX

A, B, C, D, E, F, H, I, J, L, M, N, O, P, Q, R, S, T, V, W.

Abacus, Pl. III., Fig. 1
Arcade (Norman), Pl. III., Fig. 7
Ball-Flower, Pl. VI., Fig. 3
Band, Pl. V., Figs. 10, 11
Base, Pl. III., Figs. 1, 5
Battlements, Pl. IX., Figs. 4A, 4B
Bay, Pl. XI., Fig. 2
Belfry Windows, Pl. IX., Figs. 1, 2
Boss, Pl. XII., Figs. 2, 3
Braces, Pl. X., Figs. 2, 7
Brattishing, Pl. VIII., Fig. 5
Broach-Spire, Pl. V., Fig. 7
Buttress, Pl. V., Fig. 9; Pl. VII., Fig. 10
Buttress (Diagonal), Pl. IX., Figs. 1, 2
Byzantine, Pl. I., Figs. 3 to 16
Byzantium, p. 17
Camber, Pl. X., Figs. 1, 2, p. 67
Catacombs, Pl. I., Fig. 1
Cathedral, p. 29
Centering, p. 75
Chamfer-Cusp, Pl. V., Fig. 5
Chevron, Pl. I., Fig. 4; Pl. III., Fig. 6
Chrism, Pl. I., Figs. 15, 16
Clerestory, Pl. XI., Fig. 2
Collar, Pl. X., Figs. 2, 5, 7, 8
Conventional, p. 44
Corbel Blocks, Pl. II., Fig. 3
Corbel-Table, Pl. III., Fig. 4
Crocket, Pl. V., Figs, 1, 2; Pl. VII., Figs. 10, 11, 14
Crypt, Pl. I., Fig. 2
Cushion Capital, Pl. III., Figs. 2, 8, 9
Cusp, Pl. V., Fig. 5
Cylindrical Shafts, Pl. III., Fig. 2
Detached Shafts, Pl. III., Fig. 8
Dripstone, Pl. III., Figs. 6, 8
Engaged Shafts, Pl. III., Fig. 8
Fan-Vaulting, Pl. XII., Fig. 1
Finial, Pl. V., Fig. 2; Pl. VII., Figs. 6, 10, 11; Pl. VIII., Fig. 6
Fish Symbol, Pl. I., Fig. 11
Flowing Tracery, Pl. VII., Figs. 2, 3
Flying-Buttress, Pl. VII., Fig. 10
Font (Norman), Pl. III., Fig. 7
{82}Geometrical Tracery, Pl. V., Fig. 5; Pl. VII., Fig. 1
Gothic Arch, Pl. IV., Fig. 2; Pl. V., Figs. 4, 5
Groin, Pl. XI., Figs. 3, 4, p. 75
Groundstory, Pl. XI., Fig. 2
Hammer-Beam, Pl. X., Fig. 7
Hood-Moulding, Pl. III., Figs. 6, 8
I.H.S., Pl. I., Fig. 3A
Jamb-Shaft, Pl. III., Fig. 8
Labarum, Pl. I., Figs. 15, 16
Label, Pl. VIII., Fig. 4
Lancet Windows, Pl. V., Fig. 4
Lierne-Vaulting, Pl. XI., Fig. 4; Pl. XII., Figs. 2, 3
Long-and-Short Work, Pl. II.
Mullion, Pl. IX., Figs. 1, 3, 5, 6
Nave, Pl. XI., Fig. 1
Ogee or Ogival, Pl. VI., Fig. 2
Open Timber Roof, Pl. X., Figs. 3 to 8, p. 67
Orders of Arches, Pl. III., Figs. 6, 8
Parapet, Pl. VI., Fig. 6; Pl. IX., Figs. 1 to 4
Pier, Plate III., Fig. 1
Pinnacle, Pl. VI., Fig. 6; Pl. VII., Fig. 10; Pl. IX., Figs. 1, 2, 3
Pitch of Roof, Pl. X.
Pointed Arch, pp. 37, 38
Principal and Principal Rafter, Pl. X., all Figs.
Purlin, Pl. X., Figs. 1, 2
Quadripartite Vaulting, Pl. XI., Fig. 3
Quatrefoil, Pl. I., Figs. 9, 10
Queen Post, Pl. X., Figs. 2, 7, 8
Quoin, Pl. II., Figs. 6 to 9
Rafters, Common, Pl. X., Figs. 1, 2, 4, 5, 7, 8
Respond, Pl. III., Fig. 3; Pl. XI., Fig. 2, p. 31
Reticulated Tracery, Pl. VII., Fig. 5
Sacred Monogram, Pl. I., Fig. 3A
Scallop Capital, Pl. III., Fig. 6
Scroll-Moulding, Pl. VII., Figs. 12, 13
Shaft, Pl. III., Fig. 2, p. 31
Sill, Pl. II., Fig. 3
Soffit-Cusp, Pl. V., Fig. 5
Spandril, Pl. VIII., Fig. 4, p. 60
Springer, Pl. XII., Fig. 3, detail
Spur, Pl. III., Fig. 5
Square and Circle, Pl. III., p. 30
Squinch Arches, p. 43
Stiff-Leaf, Pl. V., Fig. 8
String Courses and Dripstones, Pl. IV., Fig. 4; Pl. V., Fig. 6; Pl. VII., Fig. 12; Pl. VIII., Fig. 8
{83}Strut, Pl. X., Figs. 1, 2, 7
Studs, Pl. II., Fig. 3
Symbols, Pl. I.
Tie-Beam, Pl. X., Figs, 1, 2, 3, 8
Tooth Ornament, Pl. V., Fig. 12
Tracery Development, Pl. V., Figs. 4, 5; Pl. VII., Figs. 1 to 5
Transitional, Pl. IV.
Transom, Pl. IX., Figs. 1, 2, p. 58
Trefoil, Pl. I., Fig. 7
Triforium, Pl. XI., Fig. 2
Triquetra, Pl. I., Fig. 8; Pl. III., Fig. 9
Truss, Pl. X.
Tudor Arch, Pl. VIII., Fig. 4; Pl. IX., Fig. 6
Tudor Flower, Pl. VIII., Fig. 2
Vaulting Ribs, Pl. XII., Figs. 2, 3; Pl. XI., Figs. 3, 4
Vesica Piscis, Pl. I., Fig. 5
Wall Post, Pl. X., Figs. 3, 7, p. 68
Wave—Moulding, Pl. VII., Fig. 9
Web (Vaulting), Pl. XI., Figs. 3, 4, p. 76

PRINTED IN GREAT BRITAIN BY
BILLING AND SONS, LTD., GUILDFORD AND ESHER

*** END OF THE PROJECT GUTENBERG EBOOK ENGLISH CHURCH ARCHITECTURE OF THE MIDDLE AGES: AN ELEMENTARY HANDBOOK ***
Updated editions will replace the previous one—the old editions will be renamed.
Creating the works from print editions not protected by U.S. copyright law means that no one owns a United States copyright in these works, so the Foundation (and you!) can copy and distribute it in the United States without permission and without paying copyright royalties. Special rules, set forth in the General Terms of Use part of this license, apply to copying and distributing Project Gutenberg™ electronic works to protect the PROJECT GUTENBERG™ concept and trademark. Project Gutenberg is a registered trademark, and may not be used if you charge for an eBook, except by following the terms of the trademark license, including paying royalties for use of the Project Gutenberg trademark. If you do not charge anything for copies of this eBook, complying with the trademark license is very easy. You may use this eBook for nearly any purpose such as creation of derivative works, reports, performances and research. Project Gutenberg eBooks may be modified and printed and given away—you may do practically ANYTHING in the United States with eBooks not protected by U.S. copyright law. Redistribution is subject to the trademark license, especially commercial redistribution.
START: FULL LICENSE

## THE FULL PROJECT GUTENBERG LICENSE

PLEASE READ THIS BEFORE YOU DISTRIBUTE OR USE THIS WORK
To protect the Project Gutenberg™ mission of promoting the free distribution of electronic works, by using or distributing this work (or any other work associated in any way with the phrase “Project Gutenberg”), you agree to comply with all the terms of the Full Project Gutenberg™ License available with this file or online at www.gutenberg.org/license.
Section 1. General Terms of Use and Redistributing Project Gutenberg™ electronic works
1.A. By reading or using any part of this Project Gutenberg™ electronic work, you indicate that you have read, understand, agree to and accept all the terms of this license and intellectual property (trademark/copyright) agreement. If you do not agree to abide by all the terms of this agreement, you must cease using and return or destroy all copies of Project Gutenberg™ electronic works in your possession. If you paid a fee for obtaining a copy of or access to a Project Gutenberg™ electronic work and you do not agree to be bound by the terms of this agreement, you may obtain a refund from the person or entity to whom you paid the fee as set forth in paragraph 1.E.8.
1.B. “Project Gutenberg” is a registered trademark. It may only be used on or associated in any way with an electronic work by people who agree to be bound by the terms of this agreement. There are a few things that you can do with most Project Gutenberg™ electronic works even without complying with the full terms of this agreement. See paragraph 1.C below. There are a lot of things you can do with Project Gutenberg™ electronic works if you follow the terms of this agreement and help preserve free future access to Project Gutenberg™ electronic works. See paragraph 1.E below.
1.C. The Project Gutenberg Literary Archive Foundation (“the Foundation” or PGLAF), owns a compilation copyright in the collection of Project Gutenberg™ electronic works. Nearly all the individual works in the collection are in the public domain in the United States. If an individual work is unprotected by copyright law in the United States and you are located in the United States, we do not claim a right to prevent you from copying, distributing, performing, displaying or creating derivative works based on the work as long as all references to Project Gutenberg are removed. Of course, we hope that you will support the Project Gutenberg™ mission of promoting free access to electronic works by freely sharing Project Gutenberg™ works in compliance with the terms of this agreement for keeping the Project Gutenberg™ name associated with the work. You can easily comply with the terms of this agreement by keeping this work in the same format with its attached full Project Gutenberg™ License when you share it without charge with others.
1.D. The copyright laws of the place where you are located also govern what you can do with this work. Copyright laws in most countries are in a constant state of change. If you are outside the United States, check the laws of your country in addition to the terms of this agreement before downloading, copying, displaying, performing, distributing or creating derivative works based on this work or any other Project Gutenberg™ work. The Foundation makes no representations concerning the copyright status of any work in any country other than the United States.
1.E. Unless you have removed all references to Project Gutenberg:
1.E.1. The following sentence, with active links to, or other immediate access to, the full Project Gutenberg™ License must appear prominently whenever any copy of a Project Gutenberg™ work (any work on which the phrase “Project Gutenberg” appears, or with which the phrase “Project Gutenberg” is associated) is accessed, displayed, performed, viewed, copied or distributed:

> This eBook is for the use of anyone anywhere in the United States and most other parts of the world at no cost and with almost no restrictions whatsoever. You may copy it, give it away or re-use it under the terms of the Project Gutenberg License included with this eBook or online at www.gutenberg.org. If you are not located in the United States, you will have to check the laws of the country where you are located before using this eBook.

1.E.2. If an individual Project Gutenberg™ electronic work is derived from texts not protected by U.S. copyright law (does not contain a notice indicating that it is posted with permission of the copyright holder), the work can be copied and distributed to anyone in the United States without paying any fees or charges. If you are redistributing or providing access to a work with the phrase “Project Gutenberg” associated with or appearing on the work, you must comply either with the requirements of paragraphs 1.E.1 through 1.E.7 or obtain permission for the use of the work and the Project Gutenberg™ trademark as set forth in paragraphs 1.E.8 or 1.E.9.
1.E.3. If an individual Project Gutenberg™ electronic work is posted with the permission of the copyright holder, your use and distribution must comply with both paragraphs 1.E.1 through 1.E.7 and any additional terms imposed by the copyright holder. Additional terms will be linked to the Project Gutenberg™ License for all works posted with the permission of the copyright holder found at the beginning of this work.
1.E.4. Do not unlink or detach or remove the full Project Gutenberg™ License terms from this work, or any files containing a part of this work or any other work associated with Project Gutenberg™.
1.E.5. Do not copy, display, perform, distribute or redistribute this electronic work, or any part of this electronic work, without prominently displaying the sentence set forth in paragraph 1.E.1 with active links or immediate access to the full terms of the Project Gutenberg™ License.
1.E.6. You may convert to and distribute this work in any binary, compressed, marked up, nonproprietary or proprietary form, including any word processing or hypertext form. However, if you provide access to or distribute copies of a Project Gutenberg™ work in a format other than “Plain Vanilla ASCII” or other format used in the official version posted on the official Project Gutenberg™ website (www.gutenberg.org), you must, at no additional cost, fee or expense to the user, provide a copy, a means of exporting a copy, or a means of obtaining a copy upon request, of the work in its original “Plain Vanilla ASCII” or other form. Any alternate format must include the full Project Gutenberg™ License as specified in paragraph 1.E.1.
1.E.7. Do not charge a fee for access to, viewing, displaying, performing, copying or distributing any Project Gutenberg™ works unless you comply with paragraph 1.E.8 or 1.E.9.
1.E.8. You may charge a reasonable fee for copies of or providing access to or distributing Project Gutenberg™ electronic works provided that:

- • You pay a royalty fee of 20% of the gross profits you derive from the use of Project Gutenberg™ works calculated using the method you already use to calculate your applicable taxes. The fee is owed to the owner of the Project Gutenberg™ trademark, but he has agreed to donate royalties under this paragraph to the Project Gutenberg Literary Archive Foundation. Royalty payments must be paid within 60 days following each date on which you prepare (or are legally required to prepare) your periodic tax returns. Royalty payments should be clearly marked as such and sent to the Project Gutenberg Literary Archive Foundation at the address specified in Section 4, “Information about donations to the Project Gutenberg Literary Archive Foundation.”
- • You provide a full refund of any money paid by a user who notifies you in writing (or by e-mail) within 30 days of receipt that s/he does not agree to the terms of the full Project Gutenberg™ License. You must require such a user to return or destroy all copies of the works possessed in a physical medium and discontinue all use of and all access to other copies of Project Gutenberg™ works.
- • You provide, in accordance with paragraph 1.F.3, a full refund of any money paid for a work or a replacement copy, if a defect in the electronic work is discovered and reported to you within 90 days of receipt of the work.
- • You comply with all other terms of this agreement for free distribution of Project Gutenberg™ works.

1.E.9. If you wish to charge a fee or distribute a Project Gutenberg™ electronic work or group of works on different terms than are set forth in this agreement, you must obtain permission in writing from the Project Gutenberg Literary Archive Foundation, the manager of the Project Gutenberg™ trademark. Contact the Foundation as set forth in Section 3 below.
1.F.
1.F.1. Project Gutenberg volunteers and employees expend considerable effort to identify, do copyright research on, transcribe and proofread works not protected by U.S. copyright law in creating the Project Gutenberg™ collection. Despite these efforts, Project Gutenberg™ electronic works, and the medium on which they may be stored, may contain “Defects,” such as, but not limited to, incomplete, inaccurate or corrupt data, transcription errors, a copyright or other intellectual property infringement, a defective or damaged disk or other medium, a computer virus, or computer codes that damage or cannot be read by your equipment.
1.F.2. LIMITED WARRANTY, DISCLAIMER OF DAMAGES - Except for the “Right of Replacement or Refund” described in paragraph 1.F.3, the Project Gutenberg Literary Archive Foundation, the owner of the Project Gutenberg™ trademark, and any other party distributing a Project Gutenberg™ electronic work under this agreement, disclaim all liability to you for damages, costs and expenses, including legal fees. YOU AGREE THAT YOU HAVE NO REMEDIES FOR NEGLIGENCE, STRICT LIABILITY, BREACH OF WARRANTY OR BREACH OF CONTRACT EXCEPT THOSE PROVIDED IN PARAGRAPH 1.F.3. YOU AGREE THAT THE FOUNDATION, THE TRADEMARK OWNER, AND ANY DISTRIBUTOR UNDER THIS AGREEMENT WILL NOT BE LIABLE TO YOU FOR ACTUAL, DIRECT, INDIRECT, CONSEQUENTIAL, PUNITIVE OR INCIDENTAL DAMAGES EVEN IF YOU GIVE NOTICE OF THE POSSIBILITY OF SUCH DAMAGE.
1.F.3. LIMITED RIGHT OF REPLACEMENT OR REFUND - If you discover a defect in this electronic work within 90 days of receiving it, you can receive a refund of the money (if any) you paid for it by sending a written explanation to the person you received the work from. If you received the work on a physical medium, you must return the medium with your written explanation. The person or entity that provided you with the defective work may elect to provide a replacement copy in lieu of a refund. If you received the work electronically, the person or entity providing it to you may choose to give you a second opportunity to receive the work electronically in lieu of a refund. If the second copy is also defective, you may demand a refund in writing without further opportunities to fix the problem.
1.F.4. Except for the limited right of replacement or refund set forth in paragraph 1.F.3, this work is provided to you ‘AS-IS’, WITH NO OTHER WARRANTIES OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO WARRANTIES OF MERCHANTABILITY OR FITNESS FOR ANY PURPOSE.
1.F.5. Some states do not allow disclaimers of certain implied warranties or the exclusion or limitation of certain types of damages. If any disclaimer or limitation set forth in this agreement violates the law of the state applicable to this agreement, the agreement shall be interpreted to make the maximum disclaimer or limitation permitted by the applicable state law. The invalidity or unenforceability of any provision of this agreement shall not void the remaining provisions.
1.F.6. INDEMNITY - You agree to indemnify and hold the Foundation, the trademark owner, any agent or employee of the Foundation, anyone providing copies of Project Gutenberg™ electronic works in accordance with this agreement, and any volunteers associated with the production, promotion and distribution of Project Gutenberg™ electronic works, harmless from all liability, costs and expenses, including legal fees, that arise directly or indirectly from any of the following which you do or cause to occur: (a) distribution of this or any Project Gutenberg™ work, (b) alteration, modification, or additions or deletions to any Project Gutenberg™ work, and (c) any Defect you cause.
Section 2. Information about the Mission of Project Gutenberg™
Project Gutenberg™ is synonymous with the free distribution of electronic works in formats readable by the widest variety of computers including obsolete, old, middle-aged and new computers. It exists because of the efforts of hundreds of volunteers and donations from people in all walks of life.
Volunteers and financial support to provide volunteers with the assistance they need are critical to reaching Project Gutenberg™’s goals and ensuring that the Project Gutenberg™ collection will remain freely available for generations to come. In 2001, the Project Gutenberg Literary Archive Foundation was created to provide a secure and permanent future for Project Gutenberg™ and future generations. To learn more about the Project Gutenberg Literary Archive Foundation and how your efforts and donations can help, see Sections 3 and 4 and the Foundation information page at www.gutenberg.org.
Section 3. Information about the Project Gutenberg Literary Archive Foundation
The Project Gutenberg Literary Archive Foundation is a non-profit 501(c)(3) educational corporation organized under the laws of the state of Mississippi and granted tax exempt status by the Internal Revenue Service. The Foundation’s EIN or federal tax identification number is 64-6221541. Contributions to the Project Gutenberg Literary Archive Foundation are tax deductible to the full extent permitted by U.S. federal laws and your state’s laws.
The Foundation’s business office is located at 809 North 1500 West, Salt Lake City, UT 84116, (801) 596-1887. Email contact links and up to date contact information can be found at the Foundation’s website and official page at www.gutenberg.org/contact
Section 4. Information about Donations to the Project Gutenberg Literary Archive Foundation
Project Gutenberg™ depends upon and cannot survive without widespread public support and donations to carry out its mission of increasing the number of public domain and licensed works that can be freely distributed in machine-readable form accessible by the widest array of equipment including outdated equipment. Many small donations ($1 to $5,000) are particularly important to maintaining tax exempt status with the IRS.
The Foundation is committed to complying with the laws regulating charities and charitable donations in all 50 states of the United States. Compliance requirements are not uniform and it takes a considerable effort, much paperwork and many fees to meet and keep up with these requirements. We do not solicit donations in locations where we have not received written confirmation of compliance. To SEND DONATIONS or determine the status of compliance for any particular state visit www.gutenberg.org/donate.
While we cannot and do not solicit contributions from states where we have not met the solicitation requirements, we know of no prohibition against accepting unsolicited donations from donors in such states who approach us with offers to donate.
International donations are gratefully accepted, but we cannot make any statements concerning tax treatment of donations received from outside the United States. U.S. laws alone swamp our small staff.
Please check the Project Gutenberg web pages for current donation methods and addresses. Donations are accepted in a number of other ways including checks, online payments and credit card donations. To donate, please visit: www.gutenberg.org/donate.
Section 5. General Information About Project Gutenberg™ electronic works
Professor Michael S. Hart was the originator of the Project Gutenberg™ concept of a library of electronic works that could be freely shared with anyone. For forty years, he produced and distributed Project Gutenberg™ eBooks with only a loose network of volunteer support.
Project Gutenberg™ eBooks are often created from several printed editions, all of which are confirmed as not protected by copyright in the U.S. unless a copyright notice is included. Thus, we do not necessarily keep eBooks in compliance with any particular paper edition.
Most people start at our website which has the main PG search facility: www.gutenberg.org.
This website includes information about Project Gutenberg™, including how to make donations to the Project Gutenberg Literary Archive Foundation, how to help produce our new eBooks, and how to subscribe to our email newsletter to hear about new eBooks.